# _mm256_testz_ps, _mm_testz_ps

Performs a packed bit test of two float32 256-bit or 128-bit vectors to set the ZF flag. The corresponding Intel® AVX instruction is VTESTPS.

## Syntax

extern int _mm256_testz_ps(__m256 s1, __m256 s2);

extern int _mm_testz_ps(__m128 s1, __m128 s2);

## Arguments

s1 | first source float32 vector
s2 | second source float32 vector

## Description

Compute the bitwise AND of the two vectors s1 and s2, representing single-precision (32-bit) floating-point elements, producing an intermediate value, and set ZF to 1 if the sign bit of each 32-bit element in the intermediate value is zero, otherwise set ZF to 0. Compute the bitwise AND NOT of s1 and s2, producing an intermediate value, and set CF to 1 if the sign bit of each 32-bit element in the intermediate value is zero, otherwise set CF to 0. Return the ZF value.

### Note

Intel® Advanced Vector Extensions (Intel® AVX) instructions include a full compliment of 128-bit SIMD instructions. Such Intel® AVX instructions, with vector length of 128-bits, zeroes the upper 128 bits of the YMM register. The lower 128 bits of the YMM register is aliased to the corresponding SIMD XMM register.

## Returns

Non-zero if ZF flag is set

Zero if the ZF flag is not set

Parent topic: Intrinsics for Packed Test Operations