# _tile_stored

## Synopsis

    void _tile_stored (__tile src, void * base, int stride)

Type | Value
--- | ---
Type | Tile
Header file | `#include <immintrin.h>`
Instruction | `TILESTORED sibmem, tmm`
CPUID flags | `AMXTILE`

## Description

Store the tile specified by "src" to memory specifieid by "base" address and "stride" using the tile configuration previously configured via "_tile_loadconfig".

## Technology

AMX

## Category

Application-Targeted

## Operation

    start := tileconfig.startRow
    DO WHILE start < src.rows
    	memptr := base + start * stride
    	write_memory(memptr, src.colsb, src.row[start])
    	start := start + 1
    OD
    zero_tileconfig_start()

Parent topic: Intrinsics for Intel® Advanced Matrix Extensions AMX-TILE Instructions