# _mm256_or_ps

Performs bitwise logical OR operation on float32 vectors. The corresponding Intel® AVX instruction is VORPS.

## Syntax

extern __m256 _mm256_or_ps(__m256 m1, __m256 m2);

## Arguments

m1 | float32 vector used for the operation
m2 | float32 vector also used for the operation

## Description

Performs a bitwise logical OR of the eight packed single-precision floating-point elements (float32 elements) of the first source vector m1, and corresponding elements in the second source vector m2.

## Returns

Result of the bitwise operation.

Parent topic: Intrinsics for Bitwise Operations