# IEEE_GET_HALTING_MODE

Elemental Module Intrinsic Subroutine (Generic): Stores the halting mode for an exception.

## Module

USE, INTRINSIC :: IEEE_EXCEPTIONS

CALL IEEE_GET_HALTING_MODE (flag, halting)

flag | (Input) Must be of type TYPE (IEEE_FLAG_TYPE). It specifies one of the following IEEE flags: IEEE_DIVIDE_BY_ZERO, IEEE_INEXACT, IEEE_INVALID, IEEE_OVERFLOW, or IEEE_UNDERFLOW.
halting | (Output) Must be of type logical. If the exception in flag causes halting, the result is true; otherwise, false.

## Example

Consider the following:

    USE, INTRINSIC :: IEEE_EXCEPTIONS
    LOGICAL HALT
    ...
    CALL IEEE_GET_HALTING_MODE(IEEE_INVALID, HALT)    ! Stores the halting mode
    CALL IEEE_SET_HALTING_MODE(IEEE_INVALID, .FALSE.) ! Stops halting
    ...
    CALL IEEE_SET_HALTING_MODE(IEEE_INVALID, HALT) ! Restores halting

Parent topic: H to I

## See Also

IEEE_EXCEPTIONS Intrinsic Module
IEEE Intrinsic Modules Quick Reference Tables