ALTERA DOES NOT WARRANT THAT THE FUNCTIONS CONTAINED IN THIS PATCH 
WILL MEET YOUR REQUIREMENTS, OR THAT THE OPERATION OF THIS PATCH 
WILL BE UNINTERRUPTED OR ERROR-FREE. 

//**************************************************************** 
readme_patch_9.1_0.10.txt 
Readme file for Quartus II 9.1 Patch 0.10 
Copyright (C) Altera Corporation 2009 All right reserved. 
Patch created on November 06 2009
Patch SPR#: 327024 
SPRs fixed: 325527
//**************************************************************** 

The patch makes the following fixes to the Quartus II softwarwe:

1. Illegal mode checking for channel/PLL reconfiguration should not
   affect TX data rate switch mode.

2. Correct the address for TX data rate switch when TX data rate
   switch is used together with channel/PLL reconfig mode.

3. Reset the MIF_stage register in the altgx_reconfig after
   channel/PLL reconfig is done so that TX data rate switch performed
   after that can work properly.


Caution - You must either have previously installed the Quartus II 
          software version 9.1 or must install the Quartus II 
          software version 9.1 before installing this patch. 
          Otherwise, the patch will not be installed correctly and 
          the Quartus II software will not run properly. 
