<?xml version="1.0" encoding="UTF-8"?>
<EnsembleReport name="top" kind="system" version="14.0" fabric="QSYS">
 <!-- Format version 14.0 200 (Future versions may contain additional information.) -->
 <!-- 2014.08.05.17:38:01 -->
 <!-- A collection of modules and connections -->
 <parameter name="clockCrossingAdapter">
  <type>com.altera.sopcmodel.ensemble.EClockAdapter</type>
  <value>HANDSHAKE</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="device">
  <type>java.lang.String</type>
  <value>5AGXFB3H4F35C5</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="deviceFamily">
  <type>java.lang.String</type>
  <value>ARRIAV</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="deviceSpeedGrade">
  <type>java.lang.String</type>
  <value>5_H4</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="fabricMode">
  <type>com.altera.sopcmodel.ensemble.Ensemble$EFabricMode</type>
  <value>QSYS</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="generateLegacySim">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="generationId">
  <type>int</type>
  <value>1407285445</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="globalResetBus">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="hdlLanguage">
  <type>com.altera.entityinterfaces.moduleext.IModuleGenerateHDL$HDLLanguage</type>
  <value>VERILOG</value>
  <derived>false</derived>
  <enabled>false</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="hideFromIPCatalog">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="maxAdditionalLatency">
  <type>int</type>
  <value>0</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="projectName">
  <type>java.lang.String</type>
  <value>top.qpf</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="sopcBorderPoints">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="systemHash">
  <type>long</type>
  <value>0</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="testBenchDutName">
  <type>java.lang.String</type>
  <value></value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="timeStamp">
  <type>long</type>
  <value>0</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="useTestBenchNamingPattern">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <module
   name="pcie_reconfig_driver_0"
   kind="altera_pcie_reconfig_driver"
   version="14.0"
   path="pcie_reconfig_driver_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="INTENDED_DEVICE_FAMILY">
   <type>java.lang.String</type>
   <value>ARRIAV</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="gen123_lane_rate_mode_hwtcl">
   <type>java.lang.String</type>
   <value>Gen2 (5.0 Gbps)</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="number_of_reconfig_interfaces">
   <type>int</type>
   <value>5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_cal_busy_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_RECONFIG_XCVR_CLK_CLOCK_RATE">
   <type>java.lang.Long</type>
   <value>50000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>reconfig_xcvr_clk</sysinfo_arg>
  </parameter>
  <parameter name="AUTO_PLD_CLK_CLOCK_RATE">
   <type>java.lang.Long</type>
   <value>125000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>pld_clk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="reconfig_xcvr_clk" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>input</value>
   </assignment>
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>50000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_xcvr_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reconfig_xcvr_rst" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>input</value>
   </assignment>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>reconfig_xcvr_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_xcvr_rst</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="reconfig_mgmt" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>output</value>
   </assignment>
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>reconfig_xcvr_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reconfig_xcvr_rst</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>reconfig_mgmt_address</name>
    <direction>Output</direction>
    <width>7</width>
    <role>address</role>
   </port>
   <port>
    <name>reconfig_mgmt_read</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>reconfig_mgmt_readdata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>reconfig_mgmt_waitrequest</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>reconfig_mgmt_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>reconfig_mgmt_writedata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>alt_xcvr_reconfig_0</moduleName>
    <slaveName>reconfig_mgmt</slaveName>
    <name>alt_xcvr_reconfig_0.reconfig_mgmt</name>
    <baseAddress>0</baseAddress>
    <span>512</span>
   </memoryBlock>
  </interface>
  <interface name="hip_currentspeed" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>currentspeed</name>
    <direction>Input</direction>
    <width>2</width>
    <role>currentspeed</role>
   </port>
  </interface>
  <interface name="reconfig_busy" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_busy</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reconfig_busy</role>
   </port>
  </interface>
  <interface name="pld_clk" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>input</value>
   </assignment>
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>125000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>pld_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="cal_busy_in" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>cal_busy_in</name>
    <direction>Output</direction>
    <width>1</width>
    <role>cal_busy_in</role>
   </port>
  </interface>
  <interface name="hip_status_drv" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>derr_cor_ext_rcv_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>derr_cor_ext_rcv</role>
   </port>
   <port>
    <name>derr_cor_ext_rpl_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>derr_cor_ext_rpl</role>
   </port>
   <port>
    <name>derr_rpl_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>derr_rpl</role>
   </port>
   <port>
    <name>dlup_exit_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>dlup_exit</role>
   </port>
   <port>
    <name>ev128ns_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>ev128ns</role>
   </port>
   <port>
    <name>ev1us_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>ev1us</role>
   </port>
   <port>
    <name>hotrst_exit_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>hotrst_exit</role>
   </port>
   <port>
    <name>int_status_drv</name>
    <direction>Input</direction>
    <width>4</width>
    <role>int_status</role>
   </port>
   <port>
    <name>l2_exit_drv</name>
    <direction>Input</direction>
    <width>1</width>
    <role>l2_exit</role>
   </port>
   <port>
    <name>lane_act_drv</name>
    <direction>Input</direction>
    <width>4</width>
    <role>lane_act</role>
   </port>
   <port>
    <name>ltssmstate_drv</name>
    <direction>Input</direction>
    <width>5</width>
    <role>ltssmstate</role>
   </port>
   <port>
    <name>ko_cpl_spc_header_drv</name>
    <direction>Input</direction>
    <width>8</width>
    <role>ko_cpl_spc_header</role>
   </port>
   <port>
    <name>ko_cpl_spc_data_drv</name>
    <direction>Input</direction>
    <width>12</width>
    <role>ko_cpl_spc_data</role>
   </port>
  </interface>
 </module>
 <module
   name="alt_xcvr_reconfig_0"
   kind="alt_xcvr_reconfig"
   version="14.0"
   path="alt_xcvr_reconfig_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="device_family">
   <type>java.lang.String</type>
   <value>ARRIAV</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="number_of_reconfig_interfaces">
   <type>int</type>
   <value>5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gui_split_sizes">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_offset">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_lc">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>false</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_dcd">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_dcd_power_up">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_analog">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_eyemon">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ber_en">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_ber">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_dfe">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_adce">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_mif">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gui_enable_pll">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_pll">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>false</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gui_cal_status_port">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_MGMT_CLK_CLK_CLOCK_RATE">
   <type>java.lang.Long</type>
   <value>50000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>mgmt_clk_clk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="reconfig_busy" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>output</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_busy</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reconfig_busy</role>
   </port>
  </interface>
  <interface name="cal_busy_in" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>input</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>cal_busy_in</name>
    <direction>Input</direction>
    <width>1</width>
    <role>cal_busy_in</role>
   </port>
  </interface>
  <interface name="mgmt_clk_clk" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>50000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>mgmt_clk_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="mgmt_rst_reset" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>mgmt_clk_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>mgmt_rst_reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="reconfig_mgmt" kind="avalon_slave" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>512</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>mgmt_clk_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>mgmt_rst_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_mgmt_address</name>
    <direction>Input</direction>
    <width>7</width>
    <role>address</role>
   </port>
   <port>
    <name>reconfig_mgmt_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>reconfig_mgmt_readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>reconfig_mgmt_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>reconfig_mgmt_write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>reconfig_mgmt_writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
  </interface>
  <interface name="reconfig_to_xcvr" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>output</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_to_xcvr</name>
    <direction>Output</direction>
    <width>350</width>
    <role>reconfig_to_xcvr</role>
   </port>
  </interface>
  <interface name="reconfig_from_xcvr" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>input</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_from_xcvr</name>
    <direction>Input</direction>
    <width>230</width>
    <role>reconfig_from_xcvr</role>
   </port>
  </interface>
 </module>
 <module name="clk_0" kind="clock_source" version="14.0" path="clk_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="clockFrequency">
   <type>long</type>
   <value>50000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="clockFrequencyKnown">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="inputClockFrequency">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk_in</sysinfo_arg>
  </parameter>
  <parameter name="resetSynchronousEdges">
   <type>com.altera.sopcmodel.reset.Reset$Edges</type>
   <value>NONE</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk_in" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>qsys.ui.export_name</name>
    <value>clk</value>
   </assignment>
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>50000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>in_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="clk_in_reset" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>qsys.ui.export_name</name>
    <value>reset</value>
   </assignment>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_n</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
  <interface name="clk" kind="clock_source" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedDirectClock">
    <type>java.lang.String</type>
    <value>clk_in</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>long</type>
    <value>50000000</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>true</isStart>
   <port>
    <name>clk_out</name>
    <direction>Output</direction>
    <width>1</width>
    <role>clk</role>
   </port>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>alt_xcvr_reconfig_0</moduleName>
    <slaveName>mgmt_clk_clk</slaveName>
    <name>alt_xcvr_reconfig_0.mgmt_clk_clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>pcie_reconfig_driver_0</moduleName>
    <slaveName>reconfig_xcvr_clk</slaveName>
    <name>pcie_reconfig_driver_0.reconfig_xcvr_clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>rst_controller</moduleName>
    <slaveName>clk</slaveName>
    <name>rst_controller.clk</name>
   </clockDomainMember>
  </interface>
  <interface name="clk_reset" kind="reset_source" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value>clk_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>clk_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>reset_n_out</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
 </module>
 <module
   name="pcie_256_hip_avmm_0"
   kind="altera_pcie_256_hip_avmm"
   version="14.0"
   path="pcie_256_hip_avmm_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>testbench.partner.map.hip_ctrl</name>
   <value>pcie_tb.hip_ctrl</value>
  </assignment>
  <assignment>
   <name>testbench.partner.map.hip_pipe</name>
   <value>pcie_tb.hip_pipe</value>
  </assignment>
  <assignment>
   <name>testbench.partner.map.hip_serial</name>
   <value>pcie_tb.hip_serial</value>
  </assignment>
  <assignment>
   <name>testbench.partner.map.npor</name>
   <value>pcie_tb.npor</value>
  </assignment>
  <assignment>
   <name>testbench.partner.map.refclk</name>
   <value>pcie_tb.refclk</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.class</name>
   <value>altera_pcie_tbed</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.apps_type_hwtcl</name>
   <value>6</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.deemphasis_enable_hwtcl</name>
   <value>false</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.ecrc_check_capable_hwtcl</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.ecrc_gen_capable_hwtcl</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.enable_tl_only_sim_hwtcl</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.gen123_lane_rate_mode_hwtcl</name>
   <value>Gen3 (8.0 Gbps)</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.lane_mask_hwtcl</name>
   <value>x4</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.millisecond_cycle_count_hwtcl</name>
   <value>124250</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.pld_clk_MHz</name>
   <value>1250</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.pll_refclk_freq_hwtcl</name>
   <value>100 MHz</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.port_type_hwtcl</name>
   <value>Native endpoint</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.serial_sim_hwtcl</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.use_crc_forwarding_hwtcl</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.parameter.use_stratixv_tb_device</name>
   <value>true</value>
  </assignment>
  <assignment>
   <name>testbench.partner.pcie_tb.version</name>
   <value>14.0</value>
  </assignment>
  <parameter name="INTENDED_DEVICE_FAMILY">
   <type>java.lang.String</type>
   <value>ARRIAV</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="pcie_qsys">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="lane_mask_hwtcl">
   <type>java.lang.String</type>
   <value>x4</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gen123_lane_rate_mode_hwtcl">
   <type>java.lang.String</type>
   <value>Gen2 (5.0 Gbps)</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="app_interface_width_hwtcl">
   <type>int</type>
   <value>128</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="DMA_WIDTH">
   <type>int</type>
   <value>128</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="DMA_BE_WIDTH">
   <type>int</type>
   <value>16</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="DMA_BRST_CNT_W">
   <type>int</type>
   <value>6</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="port_type_hwtcl">
   <type>java.lang.String</type>
   <value>Native endpoint</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="pcie_spec_version_hwtcl">
   <type>java.lang.String</type>
   <value>2.1</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rxbuffer_rxreq_hwtcl">
   <type>java.lang.String</type>
   <value>Low</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="pll_refclk_freq_hwtcl">
   <type>java.lang.String</type>
   <value>100 MHz</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="set_pld_clk_x1_625MHz_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="internal_controller_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_cra_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_rxm_burst_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="in_cvp_mode_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_tl_only_sim_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="use_atx_pll_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="hip_tag_checking_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_power_on_rst_pulse_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_pcisigtest_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="SLAVE_ADDRESS_MAP_0">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>Rxm_BAR0</sysinfo_arg>
  </parameter>
  <parameter name="SLAVE_ADDRESS_MAP_1">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>Rxm_BAR1</sysinfo_arg>
  </parameter>
  <parameter name="SLAVE_ADDRESS_MAP_2">
   <type>int</type>
   <value>12</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>Rxm_BAR2</sysinfo_arg>
  </parameter>
  <parameter name="SLAVE_ADDRESS_MAP_3">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>Rxm_BAR3</sysinfo_arg>
  </parameter>
  <parameter name="SLAVE_ADDRESS_MAP_4">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>Rxm_BAR4</sysinfo_arg>
  </parameter>
  <parameter name="SLAVE_ADDRESS_MAP_5">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>Rxm_BAR5</sysinfo_arg>
  </parameter>
  <parameter name="RD_SLAVE_ADDRESS_MAP">
   <type>int</type>
   <value>15</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>dma_rd_master</sysinfo_arg>
  </parameter>
  <parameter name="WR_SLAVE_ADDRESS_MAP">
   <type>int</type>
   <value>12</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>dma_wr_master</sysinfo_arg>
  </parameter>
  <parameter name="NUM_PREFETCH_MASTERS">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar0_type_hwtcl">
   <type>int</type>
   <value>64</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar0_size_mask_hwtcl">
   <type>int</type>
   <value>9</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar0_io_space_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar0_64bit_mem_space_hwtcl">
   <type>java.lang.String</type>
   <value>Enabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar0_prefetchable_hwtcl">
   <type>java.lang.String</type>
   <value>Enabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar1_type_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar1_size_mask_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar1_io_space_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar1_prefetchable_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar2_type_hwtcl">
   <type>int</type>
   <value>64</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar2_size_mask_hwtcl">
   <type>int</type>
   <value>12</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar2_io_space_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar2_64bit_mem_space_hwtcl">
   <type>java.lang.String</type>
   <value>Enabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar2_prefetchable_hwtcl">
   <type>java.lang.String</type>
   <value>Enabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar3_type_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar3_size_mask_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar3_io_space_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar3_prefetchable_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar4_type_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar4_size_mask_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar4_io_space_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar4_64bit_mem_space_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar4_prefetchable_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar5_type_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar5_size_mask_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rd_dma_size_mask_hwtcl">
   <type>int</type>
   <value>15</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="wr_dma_size_mask_hwtcl">
   <type>int</type>
   <value>12</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar5_io_space_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bar5_prefetchable_hwtcl">
   <type>java.lang.String</type>
   <value>Disabled</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_AVALON_ADDR_B0">
   <type>int</type>
   <value>0x00000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_AVALON_ADDR_B1">
   <type>int</type>
   <value>0x00000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_AVALON_ADDR_B2">
   <type>int</type>
   <value>0x00000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_AVALON_ADDR_B3">
   <type>int</type>
   <value>0x00000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_AVALON_ADDR_B4">
   <type>int</type>
   <value>0x00000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_AVALON_ADDR_B5">
   <type>int</type>
   <value>0x00000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="fixed_address_mode">
   <type>java.lang.String</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_FIXED_AVALON_ADDR_B0">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_FIXED_AVALON_ADDR_B1">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_FIXED_AVALON_ADDR_B2">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_FIXED_AVALON_ADDR_B3">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_FIXED_AVALON_ADDR_B4">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CB_P2A_FIXED_AVALON_ADDR_B5">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vendor_id_hwtcl">
   <type>int</type>
   <value>4466</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="device_id_hwtcl">
   <type>int</type>
   <value>57347</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="revision_id_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="class_code_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="subsystem_vendor_id_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="subsystem_device_id_hwtcl">
   <type>int</type>
   <value>257</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="max_payload_size_hwtcl">
   <type>int</type>
   <value>256</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="extend_tag_field_hwtcl">
   <type>java.lang.String</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="completion_timeout_hwtcl">
   <type>java.lang.String</type>
   <value>NONE</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_completion_timeout_disable_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="use_aer_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ecrc_check_capable_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ecrc_gen_capable_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="use_crc_forwarding_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="port_link_number_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dll_active_report_support_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="surprise_down_error_support_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slotclkcfg_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msi_multi_message_capable_hwtcl">
   <type>java.lang.String</type>
   <value>4</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msi_64bit_addressing_capable_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msi_masking_capable_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msi_support_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_function_msix_support_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msix_table_size_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msix_table_offset_hwtcl">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msix_table_bir_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msix_pba_offset_hwtcl">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="msix_pba_bir_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_slot_register_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slot_power_scale_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slot_power_limit_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slot_number_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endpoint_l0_latency_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endpoint_l1_latency_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CG_COMMON_CLOCK_MODE">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="avmm_width_hwtcl">
   <type>int</type>
   <value>256</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="avmm_burst_width_hwtcl">
   <type>int</type>
   <value>7</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="CG_RXM_IRQ_NUM">
   <type>int</type>
   <value>16</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="TX_S_ADDR_WIDTH">
   <type>int</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ast_width_hwtcl">
   <type>java.lang.String</type>
   <value>Avalon-ST 128-bit</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generate_sdc_for_qsys_design_example">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="use_rx_st_be_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="use_ast_parity">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="pld_clk_MHz">
   <type>int</type>
   <value>1250</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="millisecond_cycle_count_hwtcl">
   <type>int</type>
   <value>124250</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="add_pll_to_hip_coreclkout">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="set_pll_coreclkout_slack">
   <type>int</type>
   <value>10</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="set_pll_coreclkout_cout_hwtcl">
   <type>java.lang.String</type>
   <value>NA</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="set_pll_coreclkout_cin_hwtcl">
   <type>java.lang.String</type>
   <value>NA</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="port_width_be_hwtcl">
   <type>int</type>
   <value>16</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="port_width_data_hwtcl">
   <type>int</type>
   <value>128</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="hip_reconfig_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vsec_id_hwtcl">
   <type>int</type>
   <value>40960</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vsec_rev_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="expansion_base_address_register_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="io_window_addr_width_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="prefetchable_mem_window_addr_width_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_parameter_override">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="override_tbpartner_driver_setting_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="override_rxbuffer_cred_preset">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bypass_cdc_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_rx_buffer_checking_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="disable_link_x2_support_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="wrong_device_id_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="data_pack_rx_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ltssm_1ms_timeout_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ltssm_freqlocked_check_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deskew_comma_hwtcl">
   <type>java.lang.String</type>
   <value>skp_eieos_deskw</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="device_number_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="pipex1_debug_sel_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="pclk_out_sel_hwtcl">
   <type>java.lang.String</type>
   <value>pclk</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="no_soft_reset_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="maximum_current_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d1_support_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d2_support_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d0_pme_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d1_pme_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d2_pme_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d3_hot_pme_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d3_cold_pme_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="low_priority_vc_hwtcl">
   <type>java.lang.String</type>
   <value>single_vc</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="disable_snoop_packet_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_l1_aspm_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="set_l0s_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rx_ei_l0s_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_l0s_aspm_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="aspm_config_management_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l1_exit_latency_sameclock_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l1_exit_latency_diffclock_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="hot_plug_support_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="extended_tag_reset_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="no_command_completed_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="interrupt_pin_hwtcl">
   <type>java.lang.String</type>
   <value>inta</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bridge_port_vga_enable_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bridge_port_ssid_support_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ssvid_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ssid_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="eie_before_nfts_count_hwtcl">
   <type>int</type>
   <value>4</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gen2_diffclock_nfts_count_hwtcl">
   <type>int</type>
   <value>255</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gen2_sameclock_nfts_count_hwtcl">
   <type>int</type>
   <value>255</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l0_exit_latency_sameclock_hwtcl">
   <type>int</type>
   <value>6</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l0_exit_latency_diffclock_hwtcl">
   <type>int</type>
   <value>6</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="atomic_op_routing_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="atomic_op_completer_32bit_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="atomic_op_completer_64bit_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cas_completer_128bit_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ltr_mechanism_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tph_completer_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="extended_format_field_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="atomic_malformed_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="flr_capability_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_adapter_half_rate_mode_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_clk_enable_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="register_pipe_signals_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="skp_os_gen3_count_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tx_cdc_almost_empty_hwtcl">
   <type>int</type>
   <value>5</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rx_l0s_count_idl_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cdc_dummy_insert_limit_hwtcl">
   <type>int</type>
   <value>11</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ei_delay_powerdown_count_hwtcl">
   <type>int</type>
   <value>10</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="skp_os_schedule_count_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="fc_init_timer_hwtcl">
   <type>int</type>
   <value>1024</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l01_entry_latency_hwtcl">
   <type>int</type>
   <value>31</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="flow_control_update_count_hwtcl">
   <type>int</type>
   <value>30</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="flow_control_timeout_count_hwtcl">
   <type>int</type>
   <value>200</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="retry_buffer_last_active_address_hwtcl">
   <type>int</type>
   <value>2047</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="reserved_debug_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bypass_clk_switch_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l2_async_logic_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="indicator_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="diffclock_nfts_count_hwtcl">
   <type>int</type>
   <value>128</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="sameclock_nfts_count_hwtcl">
   <type>int</type>
   <value>128</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rx_cdc_almost_full_hwtcl">
   <type>int</type>
   <value>12</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tx_cdc_almost_full_hwtcl">
   <type>int</type>
   <value>11</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="credit_buffer_allocation_aux_hwtcl">
   <type>java.lang.String</type>
   <value>absolute</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_rx_flow_ctrl_posted_header_hwtcl">
   <type>int</type>
   <value>16</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_rx_flow_ctrl_posted_data_hwtcl">
   <type>int</type>
   <value>16</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_rx_flow_ctrl_nonposted_header_hwtcl">
   <type>int</type>
   <value>16</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_rx_flow_ctrl_nonposted_data_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_rx_flow_ctrl_compl_header_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_rx_flow_ctrl_compl_data_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cpl_spc_header_hwtcl">
   <type>int</type>
   <value>195</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cpl_spc_data_hwtcl">
   <type>int</type>
   <value>781</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gen3_rxfreqlock_counter_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gen3_skip_ph2_ph3_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="g3_bypass_equlz_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cvp_data_compressed_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cvp_data_encrypted_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cvp_mode_reset_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cvp_clk_reset_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cseb_cpl_status_during_cvp_hwtcl">
   <type>java.lang.String</type>
   <value>config_retry_status</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="core_clk_sel_hwtcl">
   <type>java.lang.String</type>
   <value>pld_clk</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cvp_rate_sel_hwtcl">
   <type>java.lang.String</type>
   <value>full_rate</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="g3_dis_rx_use_prst_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="g3_dis_rx_use_prst_ep_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deemphasis_enable_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="reconfig_to_xcvr_width">
   <type>int</type>
   <value>350</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="reconfig_from_xcvr_width">
   <type>int</type>
   <value>230</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="single_rx_detect_hwtcl">
   <type>int</type>
   <value>4</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="hip_hard_reset_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="force_hrc">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="force_src">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="serial_sim_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_bypass_cdc">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_enable_rx_buffer_checking">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_disable_link_x2_support">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_wrong_device_id">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_data_pack_rx">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_ltssm_1ms_timeout">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_ltssm_freqlocked_check">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_deskew_comma">
   <type>java.lang.String</type>
   <value>com_deskw</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_device_number">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_pipex1_debug_sel">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_pclk_out_sel">
   <type>java.lang.String</type>
   <value>pclk</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_no_soft_reset">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_maximum_current">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_d1_support">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_d2_support">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_d0_pme">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_d1_pme">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_d2_pme">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_d3_hot_pme">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_d3_cold_pme">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_low_priority_vc">
   <type>java.lang.String</type>
   <value>single_vc</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_disable_snoop_packet">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_enable_l1_aspm">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_set_l0s">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_l1_exit_latency_sameclock">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_l1_exit_latency_diffclock">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_hot_plug_support">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_extended_tag_reset">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_no_command_completed">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_interrupt_pin">
   <type>java.lang.String</type>
   <value>inta</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_bridge_port_vga_enable">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_bridge_port_ssid_support">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_ssvid">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_ssid">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_eie_before_nfts_count">
   <type>int</type>
   <value>4</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_gen2_diffclock_nfts_count">
   <type>int</type>
   <value>255</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_gen2_sameclock_nfts_count">
   <type>int</type>
   <value>255</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_l0_exit_latency_sameclock">
   <type>int</type>
   <value>6</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_l0_exit_latency_diffclock">
   <type>int</type>
   <value>6</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_atomic_op_routing">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_atomic_op_completer_32bit">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_atomic_op_completer_64bit">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_cas_completer_128bit">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_ltr_mechanism">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_tph_completer">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_extended_format_field">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_atomic_malformed">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_flr_capability">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_enable_adapter_half_rate_mode">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_vc0_clk_enable">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_register_pipe_signals">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_skp_os_gen3_count">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_tx_cdc_almost_empty">
   <type>int</type>
   <value>5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_rx_l0s_count_idl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_cdc_dummy_insert_limit">
   <type>int</type>
   <value>11</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_ei_delay_powerdown_count">
   <type>int</type>
   <value>10</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_skp_os_schedule_count">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_fc_init_timer">
   <type>int</type>
   <value>1024</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_l01_entry_latency">
   <type>int</type>
   <value>31</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_flow_control_update_count">
   <type>int</type>
   <value>30</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_flow_control_timeout_count">
   <type>int</type>
   <value>200</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_retry_buffer_last_active_address">
   <type>int</type>
   <value>2047</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="advanced_default_hwtcl_reserved_debug">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="use_tl_cfg_sync_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="altpcie_avmm_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_rx_buffer_checking_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="disable_link_x2_support_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="device_number_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="pipex1_debug_sel_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="pclk_out_sel_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>pclk</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="no_soft_reset_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d1_support_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d2_support_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d0_pme_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d1_pme_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d2_pme_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d3_hot_pme_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="d3_cold_pme_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="low_priority_vc_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>single_vc</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enable_l1_aspm_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l1_exit_latency_sameclock_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l1_exit_latency_diffclock_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="hot_plug_support_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="no_command_completed_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="eie_before_nfts_count_advanced_default_hwtcl">
   <type>int</type>
   <value>4</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gen2_diffclock_nfts_count_advanced_default_hwtcl">
   <type>int</type>
   <value>255</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="gen2_sameclock_nfts_count_advanced_default_hwtcl">
   <type>int</type>
   <value>255</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deemphasis_enable_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l0_exit_latency_sameclock_advanced_default_hwtcl">
   <type>int</type>
   <value>6</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l0_exit_latency_diffclock_advanced_default_hwtcl">
   <type>int</type>
   <value>6</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="vc0_clk_enable_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="register_pipe_signals_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tx_cdc_almost_empty_advanced_default_hwtcl">
   <type>int</type>
   <value>5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rx_l0s_count_idl_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cdc_dummy_insert_limit_advanced_default_hwtcl">
   <type>int</type>
   <value>11</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ei_delay_powerdown_count_advanced_default_hwtcl">
   <type>int</type>
   <value>10</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="skp_os_schedule_count_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="fc_init_timer_advanced_default_hwtcl">
   <type>int</type>
   <value>1024</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l01_entry_latency_advanced_default_hwtcl">
   <type>int</type>
   <value>31</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="flow_control_update_count_advanced_default_hwtcl">
   <type>int</type>
   <value>30</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="flow_control_timeout_count_advanced_default_hwtcl">
   <type>int</type>
   <value>200</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="retry_buffer_last_active_address_advanced_default_hwtcl">
   <type>int</type>
   <value>255</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="reserved_debug_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="use_tl_cfg_sync_advanced_default_hwtcl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="diffclock_nfts_count_advanced_default_hwtcl">
   <type>int</type>
   <value>255</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="sameclock_nfts_count_advanced_default_hwtcl">
   <type>int</type>
   <value>255</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="l2_async_logic_advanced_default_hwtcl">
   <type>java.lang.String</type>
   <value>disable</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rx_cdc_almost_full_advanced_default_hwtcl">
   <type>int</type>
   <value>12</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tx_cdc_almost_full_advanced_default_hwtcl">
   <type>int</type>
   <value>11</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="indicator_advanced_default_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="hwtcl_override_g2_txvod">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rpre_emph_a_val_hwtcl">
   <type>int</type>
   <value>9</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rpre_emph_b_val_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rpre_emph_c_val_hwtcl">
   <type>int</type>
   <value>16</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rpre_emph_d_val_hwtcl">
   <type>int</type>
   <value>13</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rpre_emph_e_val_hwtcl">
   <type>int</type>
   <value>5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rvod_sel_a_val_hwtcl">
   <type>int</type>
   <value>42</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rvod_sel_b_val_hwtcl">
   <type>int</type>
   <value>38</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rvod_sel_c_val_hwtcl">
   <type>int</type>
   <value>38</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rvod_sel_d_val_hwtcl">
   <type>int</type>
   <value>43</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="rvod_sel_e_val_hwtcl">
   <type>int</type>
   <value>15</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rpre_emph_a_val_hwtcl">
   <type>int</type>
   <value>12</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rpre_emph_b_val_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rpre_emph_c_val_hwtcl">
   <type>int</type>
   <value>19</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rpre_emph_d_val_hwtcl">
   <type>int</type>
   <value>13</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rpre_emph_e_val_hwtcl">
   <type>int</type>
   <value>21</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rvod_sel_a_val_hwtcl">
   <type>int</type>
   <value>42</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rvod_sel_b_val_hwtcl">
   <type>int</type>
   <value>30</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rvod_sel_c_val_hwtcl">
   <type>int</type>
   <value>43</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rvod_sel_d_val_hwtcl">
   <type>int</type>
   <value>43</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="av_rvod_sel_e_val_hwtcl">
   <type>int</type>
   <value>9</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rpre_emph_a_val_hwtcl">
   <type>int</type>
   <value>11</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rpre_emph_b_val_hwtcl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rpre_emph_c_val_hwtcl">
   <type>int</type>
   <value>22</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rpre_emph_d_val_hwtcl">
   <type>int</type>
   <value>12</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rpre_emph_e_val_hwtcl">
   <type>int</type>
   <value>21</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rvod_sel_a_val_hwtcl">
   <type>int</type>
   <value>50</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rvod_sel_b_val_hwtcl">
   <type>int</type>
   <value>34</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rvod_sel_c_val_hwtcl">
   <type>int</type>
   <value>50</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rvod_sel_d_val_hwtcl">
   <type>int</type>
   <value>50</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cv_rvod_sel_e_val_hwtcl">
   <type>int</type>
   <value>9</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_REFCLK_CLOCK_RATE">
   <type>java.lang.Long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>refclk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="coreclkout" kind="clock_source" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedDirectClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>long</type>
    <value>125000000</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>true</isStart>
   <port>
    <name>coreclkout</name>
    <direction>Output</direction>
    <width>1</width>
    <role>clk</role>
   </port>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>onchip_memory2_0</moduleName>
    <slaveName>clk1</slaveName>
    <name>onchip_memory2_0.clk1</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>onchip_memory2_0</moduleName>
    <slaveName>clk2</slaveName>
    <name>onchip_memory2_0.clk2</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>pcie_reconfig_driver_0</moduleName>
    <slaveName>pld_clk</slaveName>
    <name>pcie_reconfig_driver_0.pld_clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_1</moduleName>
    <slaveName>pcie_256_hip_avmm_0_coreclkout</slaveName>
    <name>mm_interconnect_1.pcie_256_hip_avmm_0_coreclkout</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_2</moduleName>
    <slaveName>pcie_256_hip_avmm_0_coreclkout</slaveName>
    <name>mm_interconnect_2.pcie_256_hip_avmm_0_coreclkout</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_3</moduleName>
    <slaveName>pcie_256_hip_avmm_0_coreclkout</slaveName>
    <name>mm_interconnect_3.pcie_256_hip_avmm_0_coreclkout</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>rst_controller_001</moduleName>
    <slaveName>clk</slaveName>
    <name>rst_controller_001.clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>rst_translator</moduleName>
    <slaveName>clk</slaveName>
    <name>rst_translator.clk</name>
   </clockDomainMember>
  </interface>
  <interface name="refclk" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>100000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>refclk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="npor" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>npor</name>
    <direction>Input</direction>
    <width>1</width>
    <role>npor</role>
   </port>
   <port>
    <name>pin_perst</name>
    <direction>Input</direction>
    <width>1</width>
    <role>pin_perst</role>
   </port>
  </interface>
  <interface name="nreset_status" kind="reset_source" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>BOTH</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>reset_status</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
  <interface name="Rxm_BAR2" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>2</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>RxmAddress_2_o</name>
    <direction>Output</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>RxmRead_2_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>RxmWaitRequest_2_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>RxmWrite_2_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>RxmReadDataValid_2_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <port>
    <name>RxmReadData_2_i</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>RxmWriteData_2_o</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>RxmByteEnable_2_o</name>
    <direction>Output</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_1</moduleName>
    <slaveName>pcie_256_hip_avmm_0_Rxm_BAR2</slaveName>
    <name>mm_interconnect_1.pcie_256_hip_avmm_0_Rxm_BAR2</name>
    <baseAddress>0</baseAddress>
    <span>18446744073709551616</span>
   </memoryBlock>
  </interface>
  <interface name="Txs" kind="avalon_slave" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>4294967296</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>TxsAddress_i</name>
    <direction>Input</direction>
    <width>32</width>
    <role>address</role>
   </port>
   <port>
    <name>TxsChipSelect_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>TxsByteEnable_i</name>
    <direction>Input</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>TxsReadData_o</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>TxsWriteData_i</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>TxsRead_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>TxsWrite_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>TxsReadDataValid_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <port>
    <name>TxsWaitRequest_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
  </interface>
  <interface name="dma_rd_master" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>RdDmaAddress_o</name>
    <direction>Output</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>RdDmaWrite_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>RdDmaWriteData_o</name>
    <direction>Output</direction>
    <width>128</width>
    <role>writedata</role>
   </port>
   <port>
    <name>RdDmaWaitRequest_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>RdDmaBurstCount_o</name>
    <direction>Output</direction>
    <width>6</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>RdDmaWriteEnable_o</name>
    <direction>Output</direction>
    <width>16</width>
    <role>byteenable</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_1</moduleName>
    <slaveName>pcie_256_hip_avmm_0_dma_rd_master</slaveName>
    <name>mm_interconnect_1.pcie_256_hip_avmm_0_dma_rd_master</name>
    <baseAddress>0</baseAddress>
    <span>18446744073709551616</span>
   </memoryBlock>
  </interface>
  <interface name="dma_wr_master" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>WrDmaAddress_o</name>
    <direction>Output</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>WrDmaRead_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>WrDmaWaitRequest_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>WrDmaBurstCount_o</name>
    <direction>Output</direction>
    <width>6</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>WrDmaReadDataValid_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <port>
    <name>WrDmaReadData_i</name>
    <direction>Input</direction>
    <width>128</width>
    <role>readdata</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_2</moduleName>
    <slaveName>pcie_256_hip_avmm_0_dma_wr_master</slaveName>
    <name>mm_interconnect_2.pcie_256_hip_avmm_0_dma_wr_master</name>
    <baseAddress>0</baseAddress>
    <span>18446744073709551616</span>
   </memoryBlock>
  </interface>
  <interface name="wr_dts_slave" kind="avalon_slave" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>8192</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>WrDTSChipSelect_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>WrDTSWrite_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>WrDTSBurstCount_i</name>
    <direction>Input</direction>
    <width>5</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>WrDTSAddress_i</name>
    <direction>Input</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>WrDTSWriteData_i</name>
    <direction>Input</direction>
    <width>256</width>
    <role>writedata</role>
   </port>
   <port>
    <name>WrDTSWaitRequest_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
  </interface>
  <interface name="rd_dts_slave" kind="avalon_slave" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>8192</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>RdDTSChipSelect_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>RdDTSWrite_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>RdDTSBurstCount_i</name>
    <direction>Input</direction>
    <width>5</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>RdDTSAddress_i</name>
    <direction>Input</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>RdDTSWriteData_i</name>
    <direction>Input</direction>
    <width>256</width>
    <role>writedata</role>
   </port>
   <port>
    <name>RdDTSWaitRequest_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
  </interface>
  <interface name="wr_dcm_master" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>WrDCMAddress_o</name>
    <direction>Output</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>WrDCMWrite_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>WrDCMWriteData_o</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>WrDCMRead_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>WrDCMByteEnable_o</name>
    <direction>Output</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>WrDCMWaitRequest_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>WrDCMReadData_i</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>WrDCMReadDataValid_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_3</moduleName>
    <slaveName>pcie_256_hip_avmm_0_wr_dcm_master</slaveName>
    <name>mm_interconnect_3.pcie_256_hip_avmm_0_wr_dcm_master</name>
    <baseAddress>0</baseAddress>
    <span>18446744073709551616</span>
   </memoryBlock>
  </interface>
  <interface name="rd_dcm_master" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nreset_status</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>RdDCMAddress_o</name>
    <direction>Output</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>RdDCMWrite_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>RdDCMWriteData_o</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>RdDCMRead_o</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>RdDCMByteEnable_o</name>
    <direction>Output</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>RdDCMWaitRequest_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>RdDCMReadData_i</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>RdDCMReadDataValid_i</name>
    <direction>Input</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_3</moduleName>
    <slaveName>pcie_256_hip_avmm_0_rd_dcm_master</slaveName>
    <name>mm_interconnect_3.pcie_256_hip_avmm_0_rd_dcm_master</name>
    <baseAddress>0</baseAddress>
    <span>18446744073709551616</span>
   </memoryBlock>
  </interface>
  <interface name="MSI_Interface" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>Input</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>MsiIntfc_o</name>
    <direction>Output</direction>
    <width>82</width>
    <role>msi_intfc</role>
   </port>
  </interface>
  <interface name="MSIX_Interface" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>Input</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>MsixIntfc_o</name>
    <direction>Output</direction>
    <width>16</width>
    <role>msix_intfc</role>
   </port>
  </interface>
  <interface name="reconfig_to_xcvr" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>output</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_to_xcvr</name>
    <direction>Input</direction>
    <width>350</width>
    <role>reconfig_to_xcvr</role>
   </port>
  </interface>
  <interface name="reconfig_from_xcvr" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>reconfig_from_xcvr</name>
    <direction>Output</direction>
    <width>230</width>
    <role>reconfig_from_xcvr</role>
   </port>
  </interface>
  <interface name="reconfig_clk_locked" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>fixedclk_locked</name>
    <direction>Output</direction>
    <width>1</width>
    <role>fixedclk_locked</role>
   </port>
  </interface>
  <interface name="hip_serial" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>output</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>rx_in0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rx_in0</role>
   </port>
   <port>
    <name>rx_in1</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rx_in1</role>
   </port>
   <port>
    <name>rx_in2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rx_in2</role>
   </port>
   <port>
    <name>rx_in3</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rx_in3</role>
   </port>
   <port>
    <name>tx_out0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>tx_out0</role>
   </port>
   <port>
    <name>tx_out1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>tx_out1</role>
   </port>
   <port>
    <name>tx_out2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>tx_out2</role>
   </port>
   <port>
    <name>tx_out3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>tx_out3</role>
   </port>
  </interface>
  <interface name="hip_pipe" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>output</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>sim_pipe_pclk_in</name>
    <direction>Input</direction>
    <width>1</width>
    <role>sim_pipe_pclk_in</role>
   </port>
   <port>
    <name>sim_pipe_rate</name>
    <direction>Output</direction>
    <width>2</width>
    <role>sim_pipe_rate</role>
   </port>
   <port>
    <name>sim_ltssmstate</name>
    <direction>Output</direction>
    <width>5</width>
    <role>sim_ltssmstate</role>
   </port>
   <port>
    <name>eidleinfersel0</name>
    <direction>Output</direction>
    <width>3</width>
    <role>eidleinfersel0</role>
   </port>
   <port>
    <name>eidleinfersel1</name>
    <direction>Output</direction>
    <width>3</width>
    <role>eidleinfersel1</role>
   </port>
   <port>
    <name>eidleinfersel2</name>
    <direction>Output</direction>
    <width>3</width>
    <role>eidleinfersel2</role>
   </port>
   <port>
    <name>eidleinfersel3</name>
    <direction>Output</direction>
    <width>3</width>
    <role>eidleinfersel3</role>
   </port>
   <port>
    <name>powerdown0</name>
    <direction>Output</direction>
    <width>2</width>
    <role>powerdown0</role>
   </port>
   <port>
    <name>powerdown1</name>
    <direction>Output</direction>
    <width>2</width>
    <role>powerdown1</role>
   </port>
   <port>
    <name>powerdown2</name>
    <direction>Output</direction>
    <width>2</width>
    <role>powerdown2</role>
   </port>
   <port>
    <name>powerdown3</name>
    <direction>Output</direction>
    <width>2</width>
    <role>powerdown3</role>
   </port>
   <port>
    <name>rxpolarity0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>rxpolarity0</role>
   </port>
   <port>
    <name>rxpolarity1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>rxpolarity1</role>
   </port>
   <port>
    <name>rxpolarity2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>rxpolarity2</role>
   </port>
   <port>
    <name>rxpolarity3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>rxpolarity3</role>
   </port>
   <port>
    <name>txcompl0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txcompl0</role>
   </port>
   <port>
    <name>txcompl1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txcompl1</role>
   </port>
   <port>
    <name>txcompl2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txcompl2</role>
   </port>
   <port>
    <name>txcompl3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txcompl3</role>
   </port>
   <port>
    <name>txdata0</name>
    <direction>Output</direction>
    <width>8</width>
    <role>txdata0</role>
   </port>
   <port>
    <name>txdata1</name>
    <direction>Output</direction>
    <width>8</width>
    <role>txdata1</role>
   </port>
   <port>
    <name>txdata2</name>
    <direction>Output</direction>
    <width>8</width>
    <role>txdata2</role>
   </port>
   <port>
    <name>txdata3</name>
    <direction>Output</direction>
    <width>8</width>
    <role>txdata3</role>
   </port>
   <port>
    <name>txdatak0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdatak0</role>
   </port>
   <port>
    <name>txdatak1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdatak1</role>
   </port>
   <port>
    <name>txdatak2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdatak2</role>
   </port>
   <port>
    <name>txdatak3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdatak3</role>
   </port>
   <port>
    <name>txdetectrx0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdetectrx0</role>
   </port>
   <port>
    <name>txdetectrx1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdetectrx1</role>
   </port>
   <port>
    <name>txdetectrx2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdetectrx2</role>
   </port>
   <port>
    <name>txdetectrx3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdetectrx3</role>
   </port>
   <port>
    <name>txelecidle0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txelecidle0</role>
   </port>
   <port>
    <name>txelecidle1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txelecidle1</role>
   </port>
   <port>
    <name>txelecidle2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txelecidle2</role>
   </port>
   <port>
    <name>txelecidle3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txelecidle3</role>
   </port>
   <port>
    <name>txdeemph0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdeemph0</role>
   </port>
   <port>
    <name>txdeemph1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdeemph1</role>
   </port>
   <port>
    <name>txdeemph2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdeemph2</role>
   </port>
   <port>
    <name>txdeemph3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txdeemph3</role>
   </port>
   <port>
    <name>txmargin0</name>
    <direction>Output</direction>
    <width>3</width>
    <role>txmargin0</role>
   </port>
   <port>
    <name>txmargin1</name>
    <direction>Output</direction>
    <width>3</width>
    <role>txmargin1</role>
   </port>
   <port>
    <name>txmargin2</name>
    <direction>Output</direction>
    <width>3</width>
    <role>txmargin2</role>
   </port>
   <port>
    <name>txmargin3</name>
    <direction>Output</direction>
    <width>3</width>
    <role>txmargin3</role>
   </port>
   <port>
    <name>txswing0</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txswing0</role>
   </port>
   <port>
    <name>txswing1</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txswing1</role>
   </port>
   <port>
    <name>txswing2</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txswing2</role>
   </port>
   <port>
    <name>txswing3</name>
    <direction>Output</direction>
    <width>1</width>
    <role>txswing3</role>
   </port>
   <port>
    <name>phystatus0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>phystatus0</role>
   </port>
   <port>
    <name>phystatus1</name>
    <direction>Input</direction>
    <width>1</width>
    <role>phystatus1</role>
   </port>
   <port>
    <name>phystatus2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>phystatus2</role>
   </port>
   <port>
    <name>phystatus3</name>
    <direction>Input</direction>
    <width>1</width>
    <role>phystatus3</role>
   </port>
   <port>
    <name>rxdata0</name>
    <direction>Input</direction>
    <width>8</width>
    <role>rxdata0</role>
   </port>
   <port>
    <name>rxdata1</name>
    <direction>Input</direction>
    <width>8</width>
    <role>rxdata1</role>
   </port>
   <port>
    <name>rxdata2</name>
    <direction>Input</direction>
    <width>8</width>
    <role>rxdata2</role>
   </port>
   <port>
    <name>rxdata3</name>
    <direction>Input</direction>
    <width>8</width>
    <role>rxdata3</role>
   </port>
   <port>
    <name>rxdatak0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxdatak0</role>
   </port>
   <port>
    <name>rxdatak1</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxdatak1</role>
   </port>
   <port>
    <name>rxdatak2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxdatak2</role>
   </port>
   <port>
    <name>rxdatak3</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxdatak3</role>
   </port>
   <port>
    <name>rxelecidle0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxelecidle0</role>
   </port>
   <port>
    <name>rxelecidle1</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxelecidle1</role>
   </port>
   <port>
    <name>rxelecidle2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxelecidle2</role>
   </port>
   <port>
    <name>rxelecidle3</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxelecidle3</role>
   </port>
   <port>
    <name>rxstatus0</name>
    <direction>Input</direction>
    <width>3</width>
    <role>rxstatus0</role>
   </port>
   <port>
    <name>rxstatus1</name>
    <direction>Input</direction>
    <width>3</width>
    <role>rxstatus1</role>
   </port>
   <port>
    <name>rxstatus2</name>
    <direction>Input</direction>
    <width>3</width>
    <role>rxstatus2</role>
   </port>
   <port>
    <name>rxstatus3</name>
    <direction>Input</direction>
    <width>3</width>
    <role>rxstatus3</role>
   </port>
   <port>
    <name>rxvalid0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxvalid0</role>
   </port>
   <port>
    <name>rxvalid1</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxvalid1</role>
   </port>
   <port>
    <name>rxvalid2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxvalid2</role>
   </port>
   <port>
    <name>rxvalid3</name>
    <direction>Input</direction>
    <width>1</width>
    <role>rxvalid3</role>
   </port>
  </interface>
  <interface name="hip_ctrl" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>test_in</name>
    <direction>Input</direction>
    <width>32</width>
    <role>test_in</role>
   </port>
   <port>
    <name>simu_mode_pipe</name>
    <direction>Input</direction>
    <width>1</width>
    <role>simu_mode_pipe</role>
   </port>
  </interface>
  <interface name="hip_status" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>derr_cor_ext_rcv</name>
    <direction>Output</direction>
    <width>1</width>
    <role>derr_cor_ext_rcv</role>
   </port>
   <port>
    <name>derr_cor_ext_rpl</name>
    <direction>Output</direction>
    <width>1</width>
    <role>derr_cor_ext_rpl</role>
   </port>
   <port>
    <name>derr_rpl</name>
    <direction>Output</direction>
    <width>1</width>
    <role>derr_rpl</role>
   </port>
   <port>
    <name>dlup_exit</name>
    <direction>Output</direction>
    <width>1</width>
    <role>dlup_exit</role>
   </port>
   <port>
    <name>ev128ns</name>
    <direction>Output</direction>
    <width>1</width>
    <role>ev128ns</role>
   </port>
   <port>
    <name>ev1us</name>
    <direction>Output</direction>
    <width>1</width>
    <role>ev1us</role>
   </port>
   <port>
    <name>hotrst_exit</name>
    <direction>Output</direction>
    <width>1</width>
    <role>hotrst_exit</role>
   </port>
   <port>
    <name>int_status</name>
    <direction>Output</direction>
    <width>4</width>
    <role>int_status</role>
   </port>
   <port>
    <name>l2_exit</name>
    <direction>Output</direction>
    <width>1</width>
    <role>l2_exit</role>
   </port>
   <port>
    <name>lane_act</name>
    <direction>Output</direction>
    <width>4</width>
    <role>lane_act</role>
   </port>
   <port>
    <name>ltssmstate</name>
    <direction>Output</direction>
    <width>5</width>
    <role>ltssmstate</role>
   </port>
   <port>
    <name>ko_cpl_spc_header</name>
    <direction>Output</direction>
    <width>8</width>
    <role>ko_cpl_spc_header</role>
   </port>
   <port>
    <name>ko_cpl_spc_data</name>
    <direction>Output</direction>
    <width>12</width>
    <role>ko_cpl_spc_data</role>
   </port>
  </interface>
  <interface name="hip_currentspeed" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>currentspeed</name>
    <direction>Output</direction>
    <width>2</width>
    <role>currentspeed</role>
   </port>
  </interface>
  <interface name="config_tl" kind="conduit_end" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>ui.blockdiagram.direction</name>
    <value>output</value>
   </assignment>
   <parameter name="allowMultipleExportRoles">
    <type>boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>tl_cfg_add</name>
    <direction>Output</direction>
    <width>4</width>
    <role>tl_cfg_add</role>
   </port>
   <port>
    <name>tl_cfg_ctl</name>
    <direction>Output</direction>
    <width>32</width>
    <role>tl_cfg_ctl</role>
   </port>
   <port>
    <name>tl_cfg_sts</name>
    <direction>Output</direction>
    <width>53</width>
    <role>tl_cfg_sts</role>
   </port>
  </interface>
 </module>
 <module
   name="onchip_memory2_0"
   kind="altera_avalon_onchip_memory2"
   version="14.0"
   path="onchip_memory2_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>embeddedsw.CMacro.ALLOW_IN_SYSTEM_MEMORY_CONTENT_EDITOR</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.ALLOW_MRAM_SIM_CONTENTS_ONLY_FILE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CONTENTS_INFO</name>
   <value>""</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DUAL_PORT</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.GUI_RAM_BLOCK_TYPE</name>
   <value>AUTO</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.INIT_CONTENTS_FILE</name>
   <value>top_onchip_memory2_0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.INIT_MEM_CONTENT</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.INSTANCE_ID</name>
   <value>NONE</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.NON_DEFAULT_INIT_FILE_ENABLED</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.RAM_BLOCK_TYPE</name>
   <value>AUTO</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.READ_DURING_WRITE_MODE</name>
   <value>DONT_CARE</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.SINGLE_CLOCK_OP</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.SIZE_MULTIPLE</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.SIZE_VALUE</name>
   <value>4096</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.WRITABLE</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.DAT_SYM_INSTALL_DIR</name>
   <value>SIM_DIR</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.GENERATE_DAT_SYM</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.GENERATE_HEX</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.HAS_BYTE_LANE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.HEX_INSTALL_DIR</name>
   <value>QPF_DIR</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.MEM_INIT_DATA_WIDTH</name>
   <value>128</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.MEM_INIT_FILENAME</name>
   <value>top_onchip_memory2_0</value>
  </assignment>
  <assignment>
   <name>postgeneration.simulation.init_file.param_name</name>
   <value>INIT_FILE</value>
  </assignment>
  <assignment>
   <name>postgeneration.simulation.init_file.type</name>
   <value>MEM_INIT</value>
  </assignment>
  <parameter name="allowInSystemMemoryContentEditor">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="blockType">
   <type>java.lang.String</type>
   <value>AUTO</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dataWidth">
   <type>int</type>
   <value>128</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dualPort">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="initMemContent">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="initializationFileName">
   <type>java.lang.String</type>
   <value>onchip_mem.hex</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="instanceID">
   <type>java.lang.String</type>
   <value>NONE</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="memorySize">
   <type>long</type>
   <value>4096</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="readDuringWriteMode">
   <type>java.lang.String</type>
   <value>DONT_CARE</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="simAllowMRAMContentsFile">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="simMemInitOnlyFilename">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="singleClockOperation">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slave1Latency">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slave2Latency">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="useNonDefaultInitFile">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="useShallowMemBlocks">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="writable">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ecc_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetrequest_enabled">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="autoInitializationFileName">
   <type>java.lang.String</type>
   <value>top_onchip_memory2_0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>UNIQUE_ID</sysinfo_type>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>ARRIAV</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="deviceFeatures">
   <type>java.lang.String</type>
   <value>ADDRESS_STALL 1 ADVANCED_INFO 0 ALLOWS_COMPILING_OTHER_FAMILY_IP 1 ANY_QFP 0 CELL_LEVEL_BACK_ANNOTATION_DISABLED 0 COMPILER_SUPPORT 1 DSP 1 DSP_SHIFTER_BLOCK 0 DUMP_ASM_LAB_BITS_FOR_POWER 0 EMUL 0 ENABLE_ADVANCED_IO_ANALYSIS_GUI_FEATURES 1 ENABLE_PIN_PLANNER 0 ENGINEERING_SAMPLE 0 EPCS 1 ESB 0 FAKE1 0 FAKE2 0 FAKE3 0 FAMILY_LEVEL_INSTALLATION_ONLY 0 FASTEST 0 FINAL_TIMING_MODEL 0 FITTER_USE_FALLING_EDGE_DELAY 1 GENERATE_DC_ON_CURRENT_WARNING_FOR_INTERNAL_CLAMPING_DIODE 1 HARDCOPY 0 HAS_18_BIT_MULTS 1 HAS_ACE_SUPPORT 1 HAS_ACTIVE_PARALLEL_FLASH_SUPPORT 0 HAS_ADJUSTABLE_OUTPUT_IO_TIMING_MEAS_POINT 1 HAS_ADVANCED_IO_INVERTED_CORNER 1 HAS_ADVANCED_IO_POWER_SUPPORT 1 HAS_ADVANCED_IO_TIMING_SUPPORT 1 HAS_ALM_SUPPORT 1 HAS_ATOM_AND_ROUTING_POWER_MODELED_TOGETHER 0 HAS_AUTO_DERIVE_CLOCK_UNCERTAINTY_SUPPORT 1 HAS_AUTO_FIT_SUPPORT 1 HAS_BALANCED_OPT_TECHNIQUE_SUPPORT 1 HAS_BENEFICIAL_SKEW_SUPPORT 0 HAS_BITLEVEL_DRIVE_STRENGTH_CONTROL 1 HAS_BSDL_FILE_GENERATION 1 HAS_CDB_RE_NETWORK_PRESERVATION_SUPPORT 0 HAS_CGA_SUPPORT 1 HAS_CHECK_NETLIST_SUPPORT 1 HAS_CLOCK_REGION_CHECKER_ENABLED 1 HAS_CORE_JUNCTION_TEMP_DERATING 0 HAS_CROSSTALK_SUPPORT 0 HAS_CUSTOM_REGION_SUPPORT 1 HAS_DAP_JTAG_FROM_HPS 0 HAS_DATA_DRIVEN_ACVQ_HSSI_SUPPORT 1 HAS_DDB_FDI_SUPPORT 1 HAS_DESIGN_ANALYZER_SUPPORT 1 HAS_DETAILED_IO_RAIL_POWER_MODEL 1 HAS_DETAILED_LEIM_STATIC_POWER_MODEL 0 HAS_DETAILED_LE_POWER_MODEL 1 HAS_DETAILED_ROUTING_MUX_STATIC_POWER_MODEL 0 HAS_DETAILED_THERMAL_CIRCUIT_PARAMETER_SUPPORT 1 HAS_DEVICE_MIGRATION_SUPPORT 1 HAS_DIAGONAL_MIGRATION_SUPPORT 0 HAS_EMIF_TOOLKIT_SUPPORT 1 HAS_ERROR_DETECTION_SUPPORT 1 HAS_FAMILY_VARIANT_MIGRATION_SUPPORT 0 HAS_FANOUT_FREE_NODE_SUPPORT 1 HAS_FAST_FIT_SUPPORT 1 HAS_FITTER_EARLY_TIMING_ESTIMATE_SUPPORT 0 HAS_FITTER_ECO_SUPPORT 1 HAS_FIT_NETLIST_OPT_RETIME_SUPPORT 1 HAS_FIT_NETLIST_OPT_SUPPORT 1 HAS_FORMAL_VERIFICATION_SUPPORT 1 HAS_FPGA_XCHANGE_SUPPORT 1 HAS_FSAC_LUTRAM_REGISTER_PACKING_SUPPORT 1 HAS_FULL_DAT_MIN_TIMING_SUPPORT 1 HAS_FULL_INCREMENTAL_DESIGN_SUPPORT 1 HAS_FUNCTIONAL_SIMULATION_SUPPORT 0 HAS_FUNCTIONAL_VERILOG_SIMULATION_SUPPORT 1 HAS_FUNCTIONAL_VHDL_SIMULATION_SUPPORT 1 HAS_GLITCH_FILTERING_SUPPORT 1 HAS_HARDCOPYII_SUPPORT 0 HAS_HC_READY_SUPPORT 0 HAS_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_HOLD_TIME_AVOIDANCE_ACROSS_CLOCK_SPINE_SUPPORT 1 HAS_HSPICE_WRITER_SUPPORT 1 HAS_HSSI_POWER_CALCULATOR 1 HAS_IBISO_WRITER_SUPPORT 0 HAS_ICD_DATA_IP 0 HAS_INCREMENTAL_DAT_SUPPORT 1 HAS_INCREMENTAL_SYNTHESIS_SUPPORT 1 HAS_INTERFACE_PLANNER_SUPPORT 0 HAS_IO_ASSIGNMENT_ANALYSIS_SUPPORT 1 HAS_IO_DECODER 1 HAS_IO_PLACEMENT_OPTIMIZATION_SUPPORT 1 HAS_IO_SMART_RECOMPILE_SUPPORT 0 HAS_JITTER_SUPPORT 1 HAS_JTAG_SLD_HUB_SUPPORT 1 HAS_LIMITED_TCL_FITTER_SUPPORT 1 HAS_LOGICAL_FLOORPLANNER_SUPPORT 0 HAS_LOGIC_LOCK_SUPPORT 1 HAS_MICROPROCESSOR 0 HAS_MIF_SMART_COMPILE_SUPPORT 1 HAS_MINMAX_TIMING_MODELING_SUPPORT 1 HAS_MIN_TIMING_ANALYSIS_SUPPORT 1 HAS_MUX_RESTRUCTURE_SUPPORT 1 HAS_NEW_HC_FLOW_SUPPORT 0 HAS_NEW_SERDES_MAX_RESOURCE_COUNT_REPORTING_SUPPORT 0 HAS_NEW_VPR_SUPPORT 1 HAS_NONSOCKET_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_NO_HARDBLOCK_PARTITION_SUPPORT 0 HAS_NO_JTAG_USERCODE_SUPPORT 0 HAS_OPERATING_SETTINGS_AND_CONDITIONS_REPORTING_SUPPORT 1 HAS_PAD_LOCATION_ASSIGNMENT_SUPPORT 0 HAS_PARTIAL_RECONFIG_SUPPORT 1 HAS_PASSIVE_PARALLEL_SUPPORT 0 HAS_PHYSICAL_DESIGN_PLANNER_SUPPORT 0 HAS_PHYSICAL_NETLIST_OUTPUT 0 HAS_PHYSICAL_ROUTING_SUPPORT 1 HAS_PIN_SPECIFIC_VOLTAGE_SUPPORT 1 HAS_PLDM_REF_SUPPORT 0 HAS_POWER_BINNING_LIMITS_DATA 1 HAS_POWER_ESTIMATION_SUPPORT 1 HAS_PRELIMINARY_CLOCK_UNCERTAINTY_NUMBERS 0 HAS_PRE_FITTER_FPP_SUPPORT 1 HAS_PRE_FITTER_LUTRAM_NETLIST_CHECKER_ENABLED 1 HAS_PVA_SUPPORT 1 HAS_RAPID_RECOMPILE_SUPPORT 1 HAS_RCF_SUPPORT 1 HAS_RCF_SUPPORT_FOR_DEBUGGING 0 HAS_RED_BLACK_SEPARATION_SUPPORT 0 HAS_RE_LEVEL_TIMING_GRAPH_SUPPORT 1 HAS_RISEFALL_DELAY_SUPPORT 1 HAS_SIGNAL_PROBE_SUPPORT 1 HAS_SIGNAL_TAP_SUPPORT 1 HAS_SIMULATOR_SUPPORT 0 HAS_SPLIT_IO_SUPPORT 1 HAS_SPLIT_LC_SUPPORT 1 HAS_STRICT_PRESERVATION_SUPPORT 0 HAS_SYNTH_FSYN_NETLIST_OPT_SUPPORT 1 HAS_SYNTH_NETLIST_OPT_RETIME_SUPPORT 0 HAS_SYNTH_NETLIST_OPT_SUPPORT 1 HAS_TCL_FITTER_SUPPORT 0 HAS_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_TEMPLATED_REGISTER_PACKING_SUPPORT 1 HAS_TIME_BORROWING_SUPPORT 0 HAS_TIMING_DRIVEN_SYNTHESIS_SUPPORT 1 HAS_TIMING_INFO_SUPPORT 1 HAS_TIMING_OPERATING_CONDITIONS 1 HAS_TIMING_SIMULATION_SUPPORT 0 HAS_TITAN_BASED_MAC_REGISTER_PACKER_SUPPORT 1 HAS_U2B2_SUPPORT 0 HAS_USER_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_USE_FITTER_INFO_SUPPORT 0 HAS_VCCPD_POWER_RAIL 1 HAS_VERTICAL_MIGRATION_SUPPORT 1 HAS_VIEWDRAW_SYMBOL_SUPPORT 0 HAS_VIO_SUPPORT 1 HAS_VIRTUAL_DEVICES 0 HAS_WYSIWYG_DFFEAS_SUPPORT 1 HAS_XIBISO_WRITER_SUPPORT 1 IFP_USE_LEGACY_IO_CHECKER 1 INCREMENTAL_DESIGN_SUPPORTS_COMPATIBLE_CONSTRAINTS 0 INSTALLED 0 INTERNAL_POF_SUPPORT_ENABLED 0 INTERNAL_USE_ONLY 0 ISSUE_MILITARY_TEMPERATURE_WARNING 0 IS_CONFIG_ROM 0 IS_DEFAULT_FAMILY 0 IS_HARDCOPY_FAMILY 0 IS_HBGA_PACKAGE 0 IS_HIGH_CURRENT_PART 0 IS_LOW_POWER_PART 0 IS_SDM_ONLY_PACKAGE 0 LVDS_IO 1 M10K_MEMORY 1 M144K_MEMORY 1 M20K_MEMORY 0 M4K_MEMORY 0 M512_MEMORY 0 M9K_MEMORY 0 MLAB_MEMORY 1 MRAM_MEMORY 0 NOT_LISTED 0 NOT_MIGRATABLE 0 NO_FITTER_DELAY_CACHE_GENERATED 0 NO_PIN_OUT 0 NO_POF 0 NO_RPE_SUPPORT 0 NO_SUPPORT_FOR_LOGICLOCK_CONTENT_BACK_ANNOTATION 1 NO_SUPPORT_FOR_STA_CLOCK_UNCERTAINTY_CHECK 0 NO_TDC_SUPPORT 0 POSTFIT_BAK_DATABASE_EXPORT_ENABLED 1 POSTMAP_BAK_DATABASE_EXPORT_ENABLED 1 PROGRAMMER_SUPPORT 1 PVA_SUPPORTS_ONLY_SUBSET_OF_ATOMS 0 QFIT_IN_DEVELOPMENT 0 QMAP_IN_DEVELOPMENT 0 RAM_LOGICAL_NAME_CHECKING_IN_CUT_ENABLED 1 REPORTS_METASTABILITY_MTBF 1 REQUIRES_INSTALLATION_PATCH 0 REQUIRES_LIST_OF_TEMPERATURE_AND_VOLTAGE_OPERATING_CONDITIONS 1 RESERVES_SIGNAL_PROBE_PINS 0 RESOLVE_MAX_FANOUT_EARLY 1 RESOLVE_MAX_FANOUT_LATE 0 RESPECTS_FIXED_SIZED_LOCKED_LOCATION_LOGICLOCK 1 RESTRICTED_USER_SELECTION 0 RISEFALL_SUPPORT_IS_HIDDEN 0 SHOW_HIDDEN_FAMILY_IN_PROGRAMMER 0 STRICT_TIMING_DB_CHECKS 1 SUPPORTS_ADDITIONAL_OPTIONS_FOR_UNUSED_IO 1 SUPPORTS_CRC 1 SUPPORTS_DIFFERENTIAL_AIOT_BOARD_TRACE_MODEL 1 SUPPORTS_DSP_BALANCING_BACK_ANNOTATION 0 SUPPORTS_GENERATION_OF_EARLY_POWER_ESTIMATOR_FILE 1 SUPPORTS_GLOBAL_SIGNAL_BACK_ANNOTATION 1 SUPPORTS_HIPI_RETIMING 0 SUPPORTS_MAC_CHAIN_OUT_ADDER 1 SUPPORTS_RAM_PACKING_BACK_ANNOTATION 0 SUPPORTS_REG_PACKING_BACK_ANNOTATION 0 SUPPORTS_SIGNALPROBE_REGISTER_PIPELINING 1 SUPPORTS_SINGLE_ENDED_AIOT_BOARD_TRACE_MODEL 1 SUPPORTS_USER_MANUAL_LOGIC_DUPLICATION 1 TMV_RUN_CUSTOMIZABLE_VIEWER 1 TMV_RUN_INTERNAL_DETAILS 1 TMV_RUN_INTERNAL_DETAILS_ON_IO 0 TMV_RUN_INTERNAL_DETAILS_ON_IOBUF 1 TMV_RUN_INTERNAL_DETAILS_ON_LCELL 0 TMV_RUN_INTERNAL_DETAILS_ON_LRAM 0 TRANSCEIVER_3G_BLOCK 1 TRANSCEIVER_6G_BLOCK 1 USES_ACV_FOR_FLED 1 USES_ADB_FOR_BACK_ANNOTATION 1 USES_ALTERA_LNSIM 0 USES_ASIC_ROUTING_POWER_CALCULATOR 0 USES_DATA_DRIVEN_PLL_COMPUTATION_UTIL 1 USES_DEV 1 USES_ICP_FOR_ECO_FITTER 0 USES_LIBERTY_TIMING 0 USES_NETWORK_ROUTING_POWER_CALCULATOR 0 USES_POWER_SIGNAL_ACTIVITIES 1 USES_PVAFAM2 0 USES_THIRD_GENERATION_TIMING_MODELS_TIS 1 USES_U2B2_TIMING_MODELS 0 USES_XML_FORMAT_FOR_EMIF_PIN_MAP_FILE 0 USE_ADVANCED_IO_POWER_BY_DEFAULT 1 USE_ADVANCED_IO_TIMING_BY_DEFAULT 1 USE_BASE_FAMILY_DDB_PATH 0 USE_OCT_AUTO_CALIBRATION 1 USE_RELAX_IO_ASSIGNMENT_RULES 0 USE_RISEFALL_ONLY 1 USE_SEPARATE_LIST_FOR_TECH_MIGRATION 0 USE_SINGLE_COMPILER_PASS_PLL_MIF_FILE_WRITER 1 USE_TITAN_IO_BASED_IO_REGISTER_PACKER_UTIL 1 USING_28NM_OR_OLDER_TIMING_METHODOLOGY 1 WYSIWYG_BUS_WIDTH_CHECKING_IN_CUT_ENABLED 1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FEATURES</sysinfo_type>
  </parameter>
  <parameter name="derived_set_addr_width">
   <type>int</type>
   <value>8</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_set_data_width">
   <type>int</type>
   <value>128</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_gui_ram_block_type">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_is_hardcopy">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_init_file_name">
   <type>java.lang.String</type>
   <value>top_onchip_memory2_0.hex</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk1" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="s1" kind="avalon_slave" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>1</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>4096</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>4096</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>address</name>
    <direction>Input</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>clken</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clken</role>
   </port>
   <port>
    <name>chipselect</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>readdata</name>
    <direction>Output</direction>
    <width>128</width>
    <role>readdata</role>
   </port>
   <port>
    <name>writedata</name>
    <direction>Input</direction>
    <width>128</width>
    <role>writedata</role>
   </port>
   <port>
    <name>byteenable</name>
    <direction>Input</direction>
    <width>16</width>
    <role>byteenable</role>
   </port>
  </interface>
  <interface name="reset1" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
   <port>
    <name>reset_req</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
  <interface name="s2" kind="avalon_slave" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>1</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>4096</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk2</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset2</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>4096</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>address2</name>
    <direction>Input</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>chipselect2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>clken2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clken</role>
   </port>
   <port>
    <name>write2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>readdata2</name>
    <direction>Output</direction>
    <width>128</width>
    <role>readdata</role>
   </port>
   <port>
    <name>writedata2</name>
    <direction>Input</direction>
    <width>128</width>
    <role>writedata</role>
   </port>
   <port>
    <name>byteenable2</name>
    <direction>Input</direction>
    <width>16</width>
    <role>byteenable</role>
   </port>
  </interface>
  <interface name="clk2" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset2" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk2</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
   <port>
    <name>reset_req2</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
 </module>
 <module
   name="mm_interconnect_1"
   kind="altera_mm_interconnect"
   version="14.0"
   path="mm_interconnect_1">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>interconnect_id.onchip_memory2_0.s1</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.Rxm_BAR2</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.dma_rd_master</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.rd_dts_slave</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.wr_dts_slave</name>
   <value>2</value>
  </assignment>
  <parameter name="COMPOSE_CONTENTS">
   <type>java.lang.String</type>
   <value><![CDATA[add_instance {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {altera_merlin_master_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_DATA_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_READDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_READ} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_WRITE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_READDATAVALID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator} {AV_ALWAYSBURSTMAXBURST} {0};add_instance {pcie_256_hip_avmm_0_dma_rd_master_translator} {altera_merlin_master_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_DATA_W} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_BURSTCOUNT_W} {6};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_BYTEENABLE_W} {16};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {UAV_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_READDATA} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_READ} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_WRITE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_BURSTCOUNT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_SYMBOLS_PER_WORD} {16};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_CONSTANT_BURST_BEHAVIOR} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator} {AV_ALWAYSBURSTMAXBURST} {0};add_instance {onchip_memory2_0_s1_translator} {altera_merlin_slave_translator};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ADDRESS_W} {8};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_DATA_W} {128};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_DATA_W} {128};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BYTEENABLE_W} {16};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_BYTEENABLE_W} {16};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_BURSTCOUNT_W} {5};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_READLATENCY} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_READ_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READDATA} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READ} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITE} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_ADDRESS} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WAITREQUEST} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_LOCK} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_AV_CLKEN} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_SYMBOLS_PER_WORD} {16};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {pcie_256_hip_avmm_0_wr_dts_slave_translator} {altera_merlin_slave_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_ADDRESS_W} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_DATA_W} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {UAV_DATA_W} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_BURSTCOUNT_W} {5};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_BYTEENABLE_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {UAV_BYTEENABLE_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {UAV_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_READDATA} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_READ} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_WRITE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_BYTEENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_BURSTCOUNT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_AV_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_SYMBOLS_PER_WORD} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {pcie_256_hip_avmm_0_rd_dts_slave_translator} {altera_merlin_slave_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_ADDRESS_W} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_DATA_W} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {UAV_DATA_W} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_BURSTCOUNT_W} {5};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_BYTEENABLE_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {UAV_BYTEENABLE_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {UAV_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_READDATA} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_READ} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_WRITE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_BYTEENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_BURSTCOUNT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_AV_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_SYMBOLS_PER_WORD} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {altera_merlin_master_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_PROTECTION_H} {133};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_PROTECTION_L} {131};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BEGIN_BURST} {124};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BURSTWRAP_H} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BURSTWRAP_L} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BURST_SIZE_H} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BURST_SIZE_L} {117};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BURST_TYPE_H} {121};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BURST_TYPE_L} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BYTE_CNT_H} {115};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BYTE_CNT_L} {106};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_ADDR_H} {99};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_TRANS_COMPRESSED_READ} {100};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_TRANS_POSTED} {101};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_TRANS_READ} {103};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_TRANS_EXCLUSIVE} {105};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_DATA_H} {31};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_SRC_ID_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_SRC_ID_L} {126};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_DEST_ID_H} {129};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_DEST_ID_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_THREAD_ID_H} {130};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_THREAD_ID_L} {130};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_CACHE_H} {137};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_CACHE_L} {134};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_DATA_SIDEBAND_H} {123};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_DATA_SIDEBAND_L} {123};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_QOS_H} {125};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_QOS_L} {125};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_ADDR_SIDEBAND_H} {122};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_ADDR_SIDEBAND_L} {122};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_RESPONSE_STATUS_H} {139};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_RESPONSE_STATUS_L} {138};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_ORI_BURST_SIZE_L} {140};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {PKT_ORI_BURST_SIZE_H} {142};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {ST_DATA_W} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {AV_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(142:140) response_status(139:138) cache(137:134) protection(133:131) thread_id(130) dest_id(129:128) src_id(127:126) qos(125) begin_burst(124) data_sideband(123) addr_sideband(122) burst_type(121:120) burst_size(119:117) burstwrap(116) byte_cnt(115:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {ADDR_MAP} {<?xml version="1.0" encoding="UTF-8"?>
<address_map>
 <slave
   id="0"
   name="onchip_memory2_0_s1_translator.avalon_universal_slave_0"
   start="0x0000000000000000"
   end="0x00000000000001000"
   responds="1"
   user_default="0" />
</address_map>
};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {SUPPRESS_0_BYTEEN_RSP} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {ID} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {BURSTWRAP_VALUE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {CACHE_VALUE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {SECURE_ACCESS_BIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_agent} {USE_WRITERESPONSE} {0};add_instance {pcie_256_hip_avmm_0_dma_rd_master_agent} {altera_merlin_master_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_PROTECTION_H} {241};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_PROTECTION_L} {239};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BEGIN_BURST} {232};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BURSTWRAP_H} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BURSTWRAP_L} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BURST_SIZE_H} {227};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BURST_SIZE_L} {225};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BURST_TYPE_H} {229};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BURST_TYPE_L} {228};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BYTE_CNT_H} {223};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BYTE_CNT_L} {214};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_ADDR_H} {207};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_ADDR_L} {144};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_TRANS_POSTED} {209};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_TRANS_READ} {211};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_DATA_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BYTEEN_H} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_BYTEEN_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_SRC_ID_H} {235};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_SRC_ID_L} {234};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_DEST_ID_H} {237};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_DEST_ID_L} {236};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_THREAD_ID_H} {238};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_THREAD_ID_L} {238};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_CACHE_H} {245};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_CACHE_L} {242};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_DATA_SIDEBAND_H} {231};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_DATA_SIDEBAND_L} {231};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_QOS_H} {233};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_QOS_L} {233};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_ADDR_SIDEBAND_H} {230};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_ADDR_SIDEBAND_L} {230};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {ST_DATA_W} {251};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {AV_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {ADDR_MAP} {<?xml version="1.0" encoding="UTF-8"?>
<address_map>
 <slave
   id="0"
   name="onchip_memory2_0_s1_translator.avalon_universal_slave_0"
   start="0x0000000000000000"
   end="0x00000000000001000"
   responds="1"
   user_default="0" />
 <slave
   id="2"
   name="pcie_256_hip_avmm_0_wr_dts_slave_translator.avalon_universal_slave_0"
   start="0x0000000000004000"
   end="0x00000000000006000"
   responds="0"
   user_default="0" />
 <slave
   id="1"
   name="pcie_256_hip_avmm_0_rd_dts_slave_translator.avalon_universal_slave_0"
   start="0x0000000000002000"
   end="0x00000000000004000"
   responds="0"
   user_default="0" />
</address_map>
};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {SUPPRESS_0_BYTEEN_RSP} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {ID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {BURSTWRAP_VALUE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {CACHE_VALUE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {SECURE_ACCESS_BIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_agent} {USE_WRITERESPONSE} {0};add_instance {onchip_memory2_0_s1_agent} {altera_merlin_slave_agent};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DATA_H} {127};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DATA_L} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BEGIN_BURST} {232};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTEEN_H} {143};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTEEN_L} {128};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ADDR_H} {207};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ADDR_L} {144};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_POSTED} {209};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_READ} {211};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_SRC_ID_H} {235};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_SRC_ID_L} {234};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DEST_ID_H} {237};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DEST_ID_L} {236};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURSTWRAP_H} {224};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURSTWRAP_L} {224};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTE_CNT_H} {223};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTE_CNT_L} {214};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_PROTECTION_H} {241};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_PROTECTION_L} {239};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURST_SIZE_H} {227};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURST_SIZE_L} {225};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {onchip_memory2_0_s1_agent} {ST_CHANNEL_W} {3};set_instance_parameter_value {onchip_memory2_0_s1_agent} {ST_DATA_W} {251};set_instance_parameter_value {onchip_memory2_0_s1_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {AVS_BURSTCOUNT_W} {5};set_instance_parameter_value {onchip_memory2_0_s1_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {onchip_memory2_0_s1_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent} {MAX_BYTE_CNT} {16};set_instance_parameter_value {onchip_memory2_0_s1_agent} {MAX_BURSTWRAP} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent} {ID} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {USE_WRITERESPONSE} {0};add_instance {onchip_memory2_0_s1_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {BITS_PER_SYMBOL} {252};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {pcie_256_hip_avmm_0_wr_dts_slave_agent} {altera_merlin_slave_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_DATA_H} {255};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BEGIN_BURST} {376};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_TRANS_POSTED} {353};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_TRANS_WRITE} {354};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_TRANS_READ} {355};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_TRANS_LOCK} {356};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_SRC_ID_H} {379};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_SRC_ID_L} {378};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_DEST_ID_H} {381};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_DEST_ID_L} {380};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BURSTWRAP_L} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_PROTECTION_H} {385};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_PROTECTION_L} {383};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_RESPONSE_STATUS_H} {391};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_RESPONSE_STATUS_L} {390};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_ORI_BURST_SIZE_L} {392};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PKT_ORI_BURST_SIZE_H} {394};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {AVS_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {MAX_BYTE_CNT} {512};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {MAX_BURSTWRAP} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {ID} {2};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent} {USE_WRITERESPONSE} {0};add_instance {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {BITS_PER_SYMBOL} {396};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {BITS_PER_SYMBOL} {258};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {FIFO_DEPTH} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {USE_PACKETS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {EMPTY_LATENCY} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {USE_MEMORY_BLOCKS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {pcie_256_hip_avmm_0_rd_dts_slave_agent} {altera_merlin_slave_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_DATA_H} {255};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BEGIN_BURST} {376};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_TRANS_POSTED} {353};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_TRANS_WRITE} {354};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_TRANS_READ} {355};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_TRANS_LOCK} {356};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_SRC_ID_H} {379};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_SRC_ID_L} {378};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_DEST_ID_H} {381};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_DEST_ID_L} {380};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BURSTWRAP_L} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_PROTECTION_H} {385};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_PROTECTION_L} {383};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_RESPONSE_STATUS_H} {391};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_RESPONSE_STATUS_L} {390};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_ORI_BURST_SIZE_L} {392};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PKT_ORI_BURST_SIZE_H} {394};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {AVS_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {MAX_BYTE_CNT} {512};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {MAX_BURSTWRAP} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {ID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent} {USE_WRITERESPONSE} {0};add_instance {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {BITS_PER_SYMBOL} {396};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {BITS_PER_SYMBOL} {258};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {FIFO_DEPTH} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {USE_PACKETS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {EMPTY_LATENCY} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {USE_MEMORY_BLOCKS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {router} {altera_merlin_router};set_instance_parameter_value {router} {DESTINATION_ID} {0 };set_instance_parameter_value {router} {CHANNEL_ID} {1 };set_instance_parameter_value {router} {TYPE_OF_TRANSACTION} {both };set_instance_parameter_value {router} {START_ADDRESS} {0x0 };set_instance_parameter_value {router} {END_ADDRESS} {0x1000 };set_instance_parameter_value {router} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router} {SPAN_OFFSET} {};set_instance_parameter_value {router} {PKT_ADDR_H} {99};set_instance_parameter_value {router} {PKT_ADDR_L} {36};set_instance_parameter_value {router} {PKT_PROTECTION_H} {133};set_instance_parameter_value {router} {PKT_PROTECTION_L} {131};set_instance_parameter_value {router} {PKT_DEST_ID_H} {129};set_instance_parameter_value {router} {PKT_DEST_ID_L} {128};set_instance_parameter_value {router} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {router} {PKT_TRANS_READ} {103};set_instance_parameter_value {router} {ST_DATA_W} {143};set_instance_parameter_value {router} {ST_CHANNEL_W} {3};set_instance_parameter_value {router} {DECODER_TYPE} {0};set_instance_parameter_value {router} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_DESTID} {0};set_instance_parameter_value {router} {MERLIN_PACKET_FORMAT} {ori_burst_size(142:140) response_status(139:138) cache(137:134) protection(133:131) thread_id(130) dest_id(129:128) src_id(127:126) qos(125) begin_burst(124) data_sideband(123) addr_sideband(122) burst_type(121:120) burst_size(119:117) burstwrap(116) byte_cnt(115:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router} {MEMORY_ALIASING_DECODE} {0};add_instance {router_001} {altera_merlin_router};set_instance_parameter_value {router_001} {DESTINATION_ID} {0 1 2 };set_instance_parameter_value {router_001} {CHANNEL_ID} {001 100 010 };set_instance_parameter_value {router_001} {TYPE_OF_TRANSACTION} {both write write };set_instance_parameter_value {router_001} {START_ADDRESS} {0x0 0x2000 0x4000 };set_instance_parameter_value {router_001} {END_ADDRESS} {0x1000 0x4000 0x6000 };set_instance_parameter_value {router_001} {NON_SECURED_TAG} {1 1 1 };set_instance_parameter_value {router_001} {SECURED_RANGE_PAIRS} {0 0 0 };set_instance_parameter_value {router_001} {SECURED_RANGE_LIST} {0 0 0 };set_instance_parameter_value {router_001} {SPAN_OFFSET} {};set_instance_parameter_value {router_001} {PKT_ADDR_H} {207};set_instance_parameter_value {router_001} {PKT_ADDR_L} {144};set_instance_parameter_value {router_001} {PKT_PROTECTION_H} {241};set_instance_parameter_value {router_001} {PKT_PROTECTION_L} {239};set_instance_parameter_value {router_001} {PKT_DEST_ID_H} {237};set_instance_parameter_value {router_001} {PKT_DEST_ID_L} {236};set_instance_parameter_value {router_001} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {router_001} {PKT_TRANS_READ} {211};set_instance_parameter_value {router_001} {ST_DATA_W} {251};set_instance_parameter_value {router_001} {ST_CHANNEL_W} {3};set_instance_parameter_value {router_001} {DECODER_TYPE} {0};set_instance_parameter_value {router_001} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_001} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {router_001} {MEMORY_ALIASING_DECODE} {0};add_instance {router_002} {altera_merlin_router};set_instance_parameter_value {router_002} {DESTINATION_ID} {0 1 };set_instance_parameter_value {router_002} {CHANNEL_ID} {01 10 };set_instance_parameter_value {router_002} {TYPE_OF_TRANSACTION} {both write };set_instance_parameter_value {router_002} {START_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_002} {END_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_002} {NON_SECURED_TAG} {1 1 };set_instance_parameter_value {router_002} {SECURED_RANGE_PAIRS} {0 0 };set_instance_parameter_value {router_002} {SECURED_RANGE_LIST} {0 0 };set_instance_parameter_value {router_002} {SPAN_OFFSET} {};set_instance_parameter_value {router_002} {PKT_ADDR_H} {207};set_instance_parameter_value {router_002} {PKT_ADDR_L} {144};set_instance_parameter_value {router_002} {PKT_PROTECTION_H} {241};set_instance_parameter_value {router_002} {PKT_PROTECTION_L} {239};set_instance_parameter_value {router_002} {PKT_DEST_ID_H} {237};set_instance_parameter_value {router_002} {PKT_DEST_ID_L} {236};set_instance_parameter_value {router_002} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {router_002} {PKT_TRANS_READ} {211};set_instance_parameter_value {router_002} {ST_DATA_W} {251};set_instance_parameter_value {router_002} {ST_CHANNEL_W} {3};set_instance_parameter_value {router_002} {DECODER_TYPE} {1};set_instance_parameter_value {router_002} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_002} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_002} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_002} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_002} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {router_002} {MEMORY_ALIASING_DECODE} {0};add_instance {router_003} {altera_merlin_router};set_instance_parameter_value {router_003} {DESTINATION_ID} {1 };set_instance_parameter_value {router_003} {CHANNEL_ID} {1 };set_instance_parameter_value {router_003} {TYPE_OF_TRANSACTION} {write };set_instance_parameter_value {router_003} {START_ADDRESS} {0x0 };set_instance_parameter_value {router_003} {END_ADDRESS} {0x0 };set_instance_parameter_value {router_003} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router_003} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router_003} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router_003} {SPAN_OFFSET} {};set_instance_parameter_value {router_003} {PKT_ADDR_H} {351};set_instance_parameter_value {router_003} {PKT_ADDR_L} {288};set_instance_parameter_value {router_003} {PKT_PROTECTION_H} {385};set_instance_parameter_value {router_003} {PKT_PROTECTION_L} {383};set_instance_parameter_value {router_003} {PKT_DEST_ID_H} {381};set_instance_parameter_value {router_003} {PKT_DEST_ID_L} {380};set_instance_parameter_value {router_003} {PKT_TRANS_WRITE} {354};set_instance_parameter_value {router_003} {PKT_TRANS_READ} {355};set_instance_parameter_value {router_003} {ST_DATA_W} {395};set_instance_parameter_value {router_003} {ST_CHANNEL_W} {3};set_instance_parameter_value {router_003} {DECODER_TYPE} {1};set_instance_parameter_value {router_003} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_003} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_003} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_003} {DEFAULT_DESTID} {1};set_instance_parameter_value {router_003} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {router_003} {MEMORY_ALIASING_DECODE} {0};add_instance {router_004} {altera_merlin_router};set_instance_parameter_value {router_004} {DESTINATION_ID} {1 };set_instance_parameter_value {router_004} {CHANNEL_ID} {1 };set_instance_parameter_value {router_004} {TYPE_OF_TRANSACTION} {write };set_instance_parameter_value {router_004} {START_ADDRESS} {0x0 };set_instance_parameter_value {router_004} {END_ADDRESS} {0x0 };set_instance_parameter_value {router_004} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router_004} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router_004} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router_004} {SPAN_OFFSET} {};set_instance_parameter_value {router_004} {PKT_ADDR_H} {351};set_instance_parameter_value {router_004} {PKT_ADDR_L} {288};set_instance_parameter_value {router_004} {PKT_PROTECTION_H} {385};set_instance_parameter_value {router_004} {PKT_PROTECTION_L} {383};set_instance_parameter_value {router_004} {PKT_DEST_ID_H} {381};set_instance_parameter_value {router_004} {PKT_DEST_ID_L} {380};set_instance_parameter_value {router_004} {PKT_TRANS_WRITE} {354};set_instance_parameter_value {router_004} {PKT_TRANS_READ} {355};set_instance_parameter_value {router_004} {ST_DATA_W} {395};set_instance_parameter_value {router_004} {ST_CHANNEL_W} {3};set_instance_parameter_value {router_004} {DECODER_TYPE} {1};set_instance_parameter_value {router_004} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_004} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_004} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_004} {DEFAULT_DESTID} {1};set_instance_parameter_value {router_004} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {router_004} {MEMORY_ALIASING_DECODE} {0};add_instance {onchip_memory2_0_s1_burst_adapter} {altera_merlin_burst_adapter};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_ADDR_H} {207};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_ADDR_L} {144};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BEGIN_BURST} {232};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BYTE_CNT_H} {223};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BYTE_CNT_L} {214};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BYTEEN_H} {143};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BYTEEN_L} {128};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BURST_SIZE_H} {227};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BURST_SIZE_L} {225};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BURST_TYPE_H} {229};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BURST_TYPE_L} {228};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BURSTWRAP_H} {224};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_BURSTWRAP_L} {224};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PKT_TRANS_READ} {211};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {OUT_NARROW_SIZE} {0};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {IN_NARROW_SIZE} {0};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {OUT_FIXED} {0};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {OUT_COMPLETE_WRAP} {0};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {ST_DATA_W} {251};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {OUT_BYTE_CNT_H} {218};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {OUT_BURSTWRAP_H} {224};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {COMPRESSED_READ_SUPPORT} {1};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {BYTEENABLE_SYNTHESIS} {1};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {PIPE_INPUTS} {0};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {NO_WRAP_SUPPORT} {0};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {INCOMPLETE_WRAP_SUPPORT} {0};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {BURSTWRAP_CONST_MASK} {1};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {BURSTWRAP_CONST_VALUE} {1};set_instance_parameter_value {onchip_memory2_0_s1_burst_adapter} {ADAPTER_VERSION} {13.1};add_instance {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {altera_merlin_burst_adapter};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BEGIN_BURST} {376};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BURST_TYPE_H} {373};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BURST_TYPE_L} {372};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_BURSTWRAP_L} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_TRANS_WRITE} {354};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PKT_TRANS_READ} {355};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {OUT_NARROW_SIZE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {IN_NARROW_SIZE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {OUT_FIXED} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {OUT_COMPLETE_WRAP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {OUT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {OUT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {COMPRESSED_READ_SUPPORT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {BYTEENABLE_SYNTHESIS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {PIPE_INPUTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {NO_WRAP_SUPPORT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {INCOMPLETE_WRAP_SUPPORT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {BURSTWRAP_CONST_MASK} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {BURSTWRAP_CONST_VALUE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter} {ADAPTER_VERSION} {13.1};add_instance {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {altera_merlin_burst_adapter};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BEGIN_BURST} {376};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BURST_TYPE_H} {373};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BURST_TYPE_L} {372};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_BURSTWRAP_L} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_TRANS_WRITE} {354};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PKT_TRANS_READ} {355};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {OUT_NARROW_SIZE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {IN_NARROW_SIZE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {OUT_FIXED} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {OUT_COMPLETE_WRAP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {OUT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {OUT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {COMPRESSED_READ_SUPPORT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {BYTEENABLE_SYNTHESIS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {PIPE_INPUTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {NO_WRAP_SUPPORT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {INCOMPLETE_WRAP_SUPPORT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {BURSTWRAP_CONST_MASK} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {BURSTWRAP_CONST_VALUE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter} {ADAPTER_VERSION} {13.1};add_instance {cmd_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {cmd_demux} {ST_DATA_W} {143};set_instance_parameter_value {cmd_demux} {ST_CHANNEL_W} {3};set_instance_parameter_value {cmd_demux} {NUM_OUTPUTS} {1};set_instance_parameter_value {cmd_demux} {VALID_WIDTH} {1};set_instance_parameter_value {cmd_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(142:140) response_status(139:138) cache(137:134) protection(133:131) thread_id(130) dest_id(129:128) src_id(127:126) qos(125) begin_burst(124) data_sideband(123) addr_sideband(122) burst_type(121:120) burst_size(119:117) burstwrap(116) byte_cnt(115:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {cmd_demux_001} {altera_merlin_demultiplexer};set_instance_parameter_value {cmd_demux_001} {ST_DATA_W} {251};set_instance_parameter_value {cmd_demux_001} {ST_CHANNEL_W} {3};set_instance_parameter_value {cmd_demux_001} {NUM_OUTPUTS} {3};set_instance_parameter_value {cmd_demux_001} {VALID_WIDTH} {1};set_instance_parameter_value {cmd_demux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {cmd_mux} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux} {ST_DATA_W} {251};set_instance_parameter_value {cmd_mux} {ST_CHANNEL_W} {3};set_instance_parameter_value {cmd_mux} {NUM_INPUTS} {2};set_instance_parameter_value {cmd_mux} {PIPELINE_ARB} {0};set_instance_parameter_value {cmd_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {cmd_mux} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux} {ARBITRATION_SHARES} {1 1 };set_instance_parameter_value {cmd_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {cmd_mux_001} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux_001} {ST_DATA_W} {395};set_instance_parameter_value {cmd_mux_001} {ST_CHANNEL_W} {3};set_instance_parameter_value {cmd_mux_001} {NUM_INPUTS} {1};set_instance_parameter_value {cmd_mux_001} {PIPELINE_ARB} {0};set_instance_parameter_value {cmd_mux_001} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux_001} {PKT_TRANS_LOCK} {356};set_instance_parameter_value {cmd_mux_001} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux_001} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {cmd_mux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};add_instance {cmd_mux_002} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux_002} {ST_DATA_W} {395};set_instance_parameter_value {cmd_mux_002} {ST_CHANNEL_W} {3};set_instance_parameter_value {cmd_mux_002} {NUM_INPUTS} {1};set_instance_parameter_value {cmd_mux_002} {PIPELINE_ARB} {0};set_instance_parameter_value {cmd_mux_002} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux_002} {PKT_TRANS_LOCK} {356};set_instance_parameter_value {cmd_mux_002} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux_002} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {cmd_mux_002} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};add_instance {rsp_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux} {ST_DATA_W} {251};set_instance_parameter_value {rsp_demux} {ST_CHANNEL_W} {3};set_instance_parameter_value {rsp_demux} {NUM_OUTPUTS} {2};set_instance_parameter_value {rsp_demux} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {rsp_demux_001} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux_001} {ST_DATA_W} {395};set_instance_parameter_value {rsp_demux_001} {ST_CHANNEL_W} {3};set_instance_parameter_value {rsp_demux_001} {NUM_OUTPUTS} {1};set_instance_parameter_value {rsp_demux_001} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};add_instance {rsp_demux_002} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux_002} {ST_DATA_W} {395};set_instance_parameter_value {rsp_demux_002} {ST_CHANNEL_W} {3};set_instance_parameter_value {rsp_demux_002} {NUM_OUTPUTS} {1};set_instance_parameter_value {rsp_demux_002} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux_002} {MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};add_instance {rsp_mux} {altera_merlin_multiplexer};set_instance_parameter_value {rsp_mux} {ST_DATA_W} {143};set_instance_parameter_value {rsp_mux} {ST_CHANNEL_W} {3};set_instance_parameter_value {rsp_mux} {NUM_INPUTS} {1};set_instance_parameter_value {rsp_mux} {PIPELINE_ARB} {0};set_instance_parameter_value {rsp_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {rsp_mux} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {rsp_mux} {ARBITRATION_SCHEME} {no-arb};set_instance_parameter_value {rsp_mux} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {rsp_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(142:140) response_status(139:138) cache(137:134) protection(133:131) thread_id(130) dest_id(129:128) src_id(127:126) qos(125) begin_burst(124) data_sideband(123) addr_sideband(122) burst_type(121:120) burst_size(119:117) burstwrap(116) byte_cnt(115:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {rsp_mux_001} {altera_merlin_multiplexer};set_instance_parameter_value {rsp_mux_001} {ST_DATA_W} {251};set_instance_parameter_value {rsp_mux_001} {ST_CHANNEL_W} {3};set_instance_parameter_value {rsp_mux_001} {NUM_INPUTS} {3};set_instance_parameter_value {rsp_mux_001} {PIPELINE_ARB} {0};set_instance_parameter_value {rsp_mux_001} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {rsp_mux_001} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {rsp_mux_001} {ARBITRATION_SCHEME} {no-arb};set_instance_parameter_value {rsp_mux_001} {ARBITRATION_SHARES} {1 1 1 };set_instance_parameter_value {rsp_mux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_ADDR_H} {99};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_ADDR_L} {36};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_DATA_H} {31};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BYTEEN_H} {35};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BYTEEN_L} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BYTE_CNT_H} {115};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BYTE_CNT_L} {106};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {100};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BURSTWRAP_H} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BURSTWRAP_L} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BURST_SIZE_H} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BURST_SIZE_L} {117};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {139};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {138};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {105};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BURST_TYPE_H} {121};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_BURST_TYPE_L} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {140};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {142};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_ST_DATA_W} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_ADDR_H} {207};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_ADDR_L} {144};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_DATA_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BYTEEN_H} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BYTEEN_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BYTE_CNT_H} {223};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BYTE_CNT_L} {214};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BURST_SIZE_H} {227};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BURST_SIZE_L} {225};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BURST_TYPE_H} {229};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_BURST_TYPE_L} {228};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_ST_DATA_W} {251};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OPTIMIZE_FOR_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {RESPONSE_PATH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {PACKING} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(142:140) response_status(139:138) cache(137:134) protection(133:131) thread_id(130) dest_id(129:128) src_id(127:126) qos(125) begin_burst(124) data_sideband(123) addr_sideband(122) burst_type(121:120) burst_size(119:117) burstwrap(116) byte_cnt(115:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_ADDR_H} {207};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_ADDR_L} {144};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_DATA_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BYTEEN_H} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BYTEEN_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BYTE_CNT_H} {223};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BYTE_CNT_L} {214};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BURSTWRAP_H} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BURSTWRAP_L} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BURST_SIZE_H} {227};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BURST_SIZE_L} {225};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BURST_TYPE_H} {229};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_BURST_TYPE_L} {228};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_ST_DATA_W} {251};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_DATA_H} {255};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {391};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {390};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {357};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_TYPE_H} {373};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_TYPE_L} {372};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {392};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {394};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OPTIMIZE_FOR_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {RESPONSE_PATH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {PACKING} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_ADDR_H} {207};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_ADDR_L} {144};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_DATA_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BYTEEN_H} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BYTEEN_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BYTE_CNT_H} {223};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BYTE_CNT_L} {214};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BURSTWRAP_H} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BURSTWRAP_L} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BURST_SIZE_H} {227};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BURST_SIZE_L} {225};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BURST_TYPE_H} {229};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_BURST_TYPE_L} {228};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_ST_DATA_W} {251};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_DATA_H} {255};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {391};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {390};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {357};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_TYPE_H} {373};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_BURST_TYPE_L} {372};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {392};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {394};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OPTIMIZE_FOR_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {RESPONSE_PATH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {PACKING} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_ADDR_H} {207};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_ADDR_L} {144};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_DATA_H} {127};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BYTEEN_H} {143};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BYTEEN_L} {128};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BYTE_CNT_H} {223};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BYTE_CNT_L} {214};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BURSTWRAP_H} {224};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BURSTWRAP_L} {224};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BURST_SIZE_H} {227};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BURST_SIZE_L} {225};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BURST_TYPE_H} {229};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_BURST_TYPE_L} {228};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_ST_DATA_W} {251};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_ADDR_H} {99};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_ADDR_L} {36};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_DATA_H} {31};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BYTEEN_H} {35};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BYTEEN_L} {32};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BYTE_CNT_H} {115};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BYTE_CNT_L} {106};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {100};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BURST_SIZE_H} {119};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BURST_SIZE_L} {117};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {139};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {138};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {105};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BURST_TYPE_H} {121};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_BURST_TYPE_L} {120};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {140};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {142};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_ST_DATA_W} {143};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OPTIMIZE_FOR_RSP} {1};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {RESPONSE_PATH} {1};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {PACKING} {1};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(142:140) response_status(139:138) cache(137:134) protection(133:131) thread_id(130) dest_id(129:128) src_id(127:126) qos(125) begin_burst(124) data_sideband(123) addr_sideband(122) burst_type(121:120) burst_size(119:117) burstwrap(116) byte_cnt(115:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_DATA_H} {255};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURSTWRAP_L} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {391};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {390};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {357};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_TYPE_H} {373};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_TYPE_L} {372};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {392};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {394};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ADDR_H} {207};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ADDR_L} {144};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_DATA_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTEEN_H} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTEEN_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTE_CNT_H} {223};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTE_CNT_L} {214};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_SIZE_H} {227};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_SIZE_L} {225};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_TYPE_H} {229};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_TYPE_L} {228};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_ST_DATA_W} {251};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OPTIMIZE_FOR_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {RESPONSE_PATH} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {PACKING} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ADDR_H} {351};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ADDR_L} {288};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_DATA_H} {255};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTEEN_H} {287};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTEEN_L} {256};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTE_CNT_H} {367};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BYTE_CNT_L} {358};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {352};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURSTWRAP_H} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURSTWRAP_L} {368};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_SIZE_H} {371};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_SIZE_L} {369};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {391};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {390};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {357};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_TYPE_H} {373};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_BURST_TYPE_L} {372};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {392};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {394};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_ST_DATA_W} {395};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ADDR_H} {207};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ADDR_L} {144};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_DATA_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTEEN_H} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTEEN_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTE_CNT_H} {223};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BYTE_CNT_L} {214};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_SIZE_H} {227};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_SIZE_L} {225};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {247};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {246};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_TYPE_H} {229};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_BURST_TYPE_L} {228};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {248};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {250};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_ST_DATA_W} {251};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {ST_CHANNEL_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OPTIMIZE_FOR_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {RESPONSE_PATH} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {PACKING} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(394:392) response_status(391:390) cache(389:386) protection(385:383) thread_id(382) dest_id(381:380) src_id(379:378) qos(377) begin_burst(376) data_sideband(375) addr_sideband(374) burst_type(373:372) burst_size(371:369) burstwrap(368) byte_cnt(367:358) trans_exclusive(357) trans_lock(356) trans_read(355) trans_write(354) trans_posted(353) trans_compressed_read(352) addr(351:288) byteen(287:256) data(255:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(250:248) response_status(247:246) cache(245:242) protection(241:239) thread_id(238) dest_id(237:236) src_id(235:234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {onchip_memory2_0_reset1_reset_bridge} {altera_reset_bridge};set_instance_parameter_value {onchip_memory2_0_reset1_reset_bridge} {ACTIVE_LOW_RESET} {0};set_instance_parameter_value {onchip_memory2_0_reset1_reset_bridge} {SYNCHRONOUS_EDGES} {deassert};set_instance_parameter_value {onchip_memory2_0_reset1_reset_bridge} {NUM_RESET_OUTPUTS} {1};add_instance {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {altera_clock_bridge};set_instance_parameter_value {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {EXPLICIT_CLOCK_RATE} {125000000};set_instance_parameter_value {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {NUM_CLOCK_OUTPUTS} {1};add_connection {pcie_256_hip_avmm_0_Rxm_BAR2_translator.avalon_universal_master_0} {pcie_256_hip_avmm_0_Rxm_BAR2_agent.av} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_Rxm_BAR2_agent.av} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_Rxm_BAR2_agent.av} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_Rxm_BAR2_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_Rxm_BAR2_agent.av} {defaultConnection} {false};add_connection {rsp_mux.src} {pcie_256_hip_avmm_0_Rxm_BAR2_agent.rp} {avalon_streaming};preview_set_connection_tag {rsp_mux.src/pcie_256_hip_avmm_0_Rxm_BAR2_agent.rp} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_dma_rd_master_translator.avalon_universal_master_0} {pcie_256_hip_avmm_0_dma_rd_master_agent.av} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_dma_rd_master_agent.av} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_dma_rd_master_agent.av} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_dma_rd_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_dma_rd_master_agent.av} {defaultConnection} {false};add_connection {rsp_mux_001.src} {pcie_256_hip_avmm_0_dma_rd_master_agent.rp} {avalon_streaming};preview_set_connection_tag {rsp_mux_001.src/pcie_256_hip_avmm_0_dma_rd_master_agent.rp} {qsys_mm.response};add_connection {onchip_memory2_0_s1_agent.m0} {onchip_memory2_0_s1_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {onchip_memory2_0_s1_agent.m0/onchip_memory2_0_s1_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {onchip_memory2_0_s1_agent.m0/onchip_memory2_0_s1_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {onchip_memory2_0_s1_agent.m0/onchip_memory2_0_s1_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {onchip_memory2_0_s1_agent.rf_source} {onchip_memory2_0_s1_agent_rsp_fifo.in} {avalon_streaming};add_connection {onchip_memory2_0_s1_agent_rsp_fifo.out} {onchip_memory2_0_s1_agent.rf_sink} {avalon_streaming};add_connection {onchip_memory2_0_s1_agent.rdata_fifo_src} {onchip_memory2_0_s1_agent.rdata_fifo_sink} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_agent.m0} {pcie_256_hip_avmm_0_wr_dts_slave_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent.m0/pcie_256_hip_avmm_0_wr_dts_slave_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent.m0/pcie_256_hip_avmm_0_wr_dts_slave_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_wr_dts_slave_agent.m0/pcie_256_hip_avmm_0_wr_dts_slave_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_agent.rf_source} {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo.in} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo.out} {pcie_256_hip_avmm_0_wr_dts_slave_agent.rf_sink} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_agent.rdata_fifo_src} {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo.in} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo.out} {pcie_256_hip_avmm_0_wr_dts_slave_agent.rdata_fifo_sink} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_agent.m0} {pcie_256_hip_avmm_0_rd_dts_slave_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent.m0/pcie_256_hip_avmm_0_rd_dts_slave_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent.m0/pcie_256_hip_avmm_0_rd_dts_slave_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_rd_dts_slave_agent.m0/pcie_256_hip_avmm_0_rd_dts_slave_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_agent.rf_source} {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo.in} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo.out} {pcie_256_hip_avmm_0_rd_dts_slave_agent.rf_sink} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_agent.rdata_fifo_src} {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo.in} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo.out} {pcie_256_hip_avmm_0_rd_dts_slave_agent.rdata_fifo_sink} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_Rxm_BAR2_agent.cp} {router.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_Rxm_BAR2_agent.cp/router.sink} {qsys_mm.command};add_connection {router.src} {cmd_demux.sink} {avalon_streaming};preview_set_connection_tag {router.src/cmd_demux.sink} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_dma_rd_master_agent.cp} {router_001.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_dma_rd_master_agent.cp/router_001.sink} {qsys_mm.command};add_connection {router_001.src} {cmd_demux_001.sink} {avalon_streaming};preview_set_connection_tag {router_001.src/cmd_demux_001.sink} {qsys_mm.command};add_connection {onchip_memory2_0_s1_agent.rp} {router_002.sink} {avalon_streaming};preview_set_connection_tag {onchip_memory2_0_s1_agent.rp/router_002.sink} {qsys_mm.response};add_connection {router_002.src} {rsp_demux.sink} {avalon_streaming};preview_set_connection_tag {router_002.src/rsp_demux.sink} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_agent.rp} {router_003.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_wr_dts_slave_agent.rp/router_003.sink} {qsys_mm.response};add_connection {router_003.src} {rsp_demux_001.sink} {avalon_streaming};preview_set_connection_tag {router_003.src/rsp_demux_001.sink} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_agent.rp} {router_004.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_rd_dts_slave_agent.rp/router_004.sink} {qsys_mm.response};add_connection {router_004.src} {rsp_demux_002.sink} {avalon_streaming};preview_set_connection_tag {router_004.src/rsp_demux_002.sink} {qsys_mm.response};add_connection {cmd_mux.src} {onchip_memory2_0_s1_burst_adapter.sink0} {avalon_streaming};preview_set_connection_tag {cmd_mux.src/onchip_memory2_0_s1_burst_adapter.sink0} {qsys_mm.command};add_connection {onchip_memory2_0_s1_burst_adapter.source0} {onchip_memory2_0_s1_agent.cp} {avalon_streaming};preview_set_connection_tag {onchip_memory2_0_s1_burst_adapter.source0/onchip_memory2_0_s1_agent.cp} {qsys_mm.command};add_connection {cmd_mux_001.src} {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter.sink0} {avalon_streaming};preview_set_connection_tag {cmd_mux_001.src/pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter.sink0} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter.source0} {pcie_256_hip_avmm_0_wr_dts_slave_agent.cp} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter.source0/pcie_256_hip_avmm_0_wr_dts_slave_agent.cp} {qsys_mm.command};add_connection {cmd_mux_002.src} {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter.sink0} {avalon_streaming};preview_set_connection_tag {cmd_mux_002.src/pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter.sink0} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter.source0} {pcie_256_hip_avmm_0_rd_dts_slave_agent.cp} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter.source0/pcie_256_hip_avmm_0_rd_dts_slave_agent.cp} {qsys_mm.command};add_connection {cmd_demux_001.src0} {cmd_mux.sink1} {avalon_streaming};preview_set_connection_tag {cmd_demux_001.src0/cmd_mux.sink1} {qsys_mm.command};add_connection {rsp_demux.src1} {rsp_mux_001.sink0} {avalon_streaming};preview_set_connection_tag {rsp_demux.src1/rsp_mux_001.sink0} {qsys_mm.response};add_connection {cmd_demux.src0} {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {cmd_demux.src0/pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter.sink} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter.src} {cmd_mux.sink0} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter.src/cmd_mux.sink0} {qsys_mm.command};add_connection {cmd_demux_001.src1} {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {cmd_demux_001.src1/pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter.sink} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter.src} {cmd_mux_001.sink0} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter.src/cmd_mux_001.sink0} {qsys_mm.command};add_connection {cmd_demux_001.src2} {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {cmd_demux_001.src2/pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter.sink} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter.src} {cmd_mux_002.sink0} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter.src/cmd_mux_002.sink0} {qsys_mm.command};add_connection {rsp_demux.src0} {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {rsp_demux.src0/onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter.sink} {qsys_mm.response};add_connection {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter.src} {rsp_mux.sink0} {avalon_streaming};preview_set_connection_tag {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter.src/rsp_mux.sink0} {qsys_mm.response};add_connection {rsp_demux_001.src0} {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {rsp_demux_001.src0/pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.sink} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.src} {rsp_mux_001.sink1} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.src/rsp_mux_001.sink1} {qsys_mm.response};add_connection {rsp_demux_002.src0} {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {rsp_demux_002.src0/pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.sink} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.src} {rsp_mux_001.sink2} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.src/rsp_mux_001.sink2} {qsys_mm.response};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_Rxm_BAR2_translator.reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_dma_rd_master_translator.reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {onchip_memory2_0_s1_translator.reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dts_slave_translator.reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dts_slave_translator.reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_Rxm_BAR2_agent.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_dma_rd_master_agent.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {onchip_memory2_0_s1_agent.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {onchip_memory2_0_s1_agent_rsp_fifo.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dts_slave_agent.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dts_slave_agent.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {router.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {router_001.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {router_002.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {router_003.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {router_004.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {onchip_memory2_0_s1_burst_adapter.cr0_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter.cr0_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter.cr0_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {cmd_demux.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {cmd_demux_001.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {cmd_mux.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {cmd_mux_001.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {cmd_mux_002.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {rsp_demux.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {rsp_demux_001.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {rsp_demux_002.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {rsp_mux.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {rsp_mux_001.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.clk_reset} {reset};add_connection {onchip_memory2_0_reset1_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_Rxm_BAR2_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_dma_rd_master_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s1_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dts_slave_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dts_slave_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_Rxm_BAR2_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_dma_rd_master_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s1_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s1_agent_rsp_fifo.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dts_slave_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dts_slave_agent_rsp_fifo.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dts_slave_agent_rdata_fifo.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dts_slave_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dts_slave_agent_rsp_fifo.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dts_slave_agent_rdata_fifo.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router_002.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router_003.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router_004.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s1_burst_adapter.cr0} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dts_slave_burst_adapter.cr0} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dts_slave_burst_adapter.cr0} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_demux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_mux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_demux_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_mux_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_mux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_demux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_mux_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_demux_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_mux_002.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_demux_002.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_Rxm_BAR2_to_onchip_memory2_0_s1_cmd_width_adapter.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_wr_dts_slave_cmd_width_adapter.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_dma_rd_master_to_pcie_256_hip_avmm_0_rd_dts_slave_cmd_width_adapter.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s1_to_pcie_256_hip_avmm_0_Rxm_BAR2_rsp_width_adapter.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dts_slave_to_pcie_256_hip_avmm_0_dma_rd_master_rsp_width_adapter.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_reset1_reset_bridge.clk} {clock};add_interface {pcie_256_hip_avmm_0_coreclkout} {clock} {slave};set_interface_property {pcie_256_hip_avmm_0_coreclkout} {EXPORT_OF} {pcie_256_hip_avmm_0_coreclkout_clock_bridge.in_clk};add_interface {onchip_memory2_0_reset1_reset_bridge_in_reset} {reset} {slave};set_interface_property {onchip_memory2_0_reset1_reset_bridge_in_reset} {EXPORT_OF} {onchip_memory2_0_reset1_reset_bridge.in_reset};add_interface {pcie_256_hip_avmm_0_dma_rd_master} {avalon} {slave};set_interface_property {pcie_256_hip_avmm_0_dma_rd_master} {EXPORT_OF} {pcie_256_hip_avmm_0_dma_rd_master_translator.avalon_anti_master_0};add_interface {pcie_256_hip_avmm_0_Rxm_BAR2} {avalon} {slave};set_interface_property {pcie_256_hip_avmm_0_Rxm_BAR2} {EXPORT_OF} {pcie_256_hip_avmm_0_Rxm_BAR2_translator.avalon_anti_master_0};add_interface {onchip_memory2_0_s1} {avalon} {master};set_interface_property {onchip_memory2_0_s1} {EXPORT_OF} {onchip_memory2_0_s1_translator.avalon_anti_slave_0};add_interface {pcie_256_hip_avmm_0_rd_dts_slave} {avalon} {master};set_interface_property {pcie_256_hip_avmm_0_rd_dts_slave} {EXPORT_OF} {pcie_256_hip_avmm_0_rd_dts_slave_translator.avalon_anti_slave_0};add_interface {pcie_256_hip_avmm_0_wr_dts_slave} {avalon} {master};set_interface_property {pcie_256_hip_avmm_0_wr_dts_slave} {EXPORT_OF} {pcie_256_hip_avmm_0_wr_dts_slave_translator.avalon_anti_slave_0};set_module_assignment {interconnect_id.onchip_memory2_0.s1} {0};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.Rxm_BAR2} {0};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.dma_rd_master} {1};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.rd_dts_slave} {1};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.wr_dts_slave} {2};]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_DEVICE_FAMILY">
   <type>java.lang.String</type>
   <value>ARRIAV</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="AUTO_DEVICE">
   <type>java.lang.String</type>
   <value>5AGXFB3H4F35C5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE</sysinfo_type>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>Arria V</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface
     name="pcie_256_hip_avmm_0_coreclkout"
     kind="clock_sink"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_coreclkout_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface
     name="onchip_memory2_0_reset1_reset_bridge_in_reset"
     kind="reset_sink"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>onchip_memory2_0_reset1_reset_bridge_in_reset_reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_dma_rd_master"
     kind="avalon_slave"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>merlin.flow.avalon_universal_master_0</name>
    <value>avalon_universal_master_0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>18446744073709551616</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>onchip_memory2_0_reset1_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_dma_rd_master_address</name>
    <direction>Input</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_rd_master_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_rd_master_burstcount</name>
    <direction>Input</direction>
    <width>6</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_rd_master_byteenable</name>
    <direction>Input</direction>
    <width>16</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_rd_master_write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_rd_master_writedata</name>
    <direction>Input</direction>
    <width>128</width>
    <role>writedata</role>
   </port>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_Rxm_BAR2"
     kind="avalon_slave"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>merlin.flow.avalon_universal_master_0</name>
    <value>avalon_universal_master_0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>18446744073709551616</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>onchip_memory2_0_reset1_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_address</name>
    <direction>Input</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_byteenable</name>
    <direction>Input</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_readdatavalid</name>
    <direction>Output</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Rxm_BAR2_writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
  </interface>
  <interface name="onchip_memory2_0_s1" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>onchip_memory2_0_reset1_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>onchip_memory2_0_s1_address</name>
    <direction>Output</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_readdata</name>
    <direction>Input</direction>
    <width>128</width>
    <role>readdata</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_writedata</name>
    <direction>Output</direction>
    <width>128</width>
    <role>writedata</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_byteenable</name>
    <direction>Output</direction>
    <width>16</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_clken</name>
    <direction>Output</direction>
    <width>1</width>
    <role>clken</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>onchip_memory2_0</moduleName>
    <slaveName>s1</slaveName>
    <name>onchip_memory2_0.s1</name>
    <baseAddress>0</baseAddress>
    <span>4096</span>
   </memoryBlock>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_rd_dts_slave"
     kind="avalon_master"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>onchip_memory2_0_reset1_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dts_slave_address</name>
    <direction>Output</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dts_slave_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dts_slave_writedata</name>
    <direction>Output</direction>
    <width>256</width>
    <role>writedata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dts_slave_burstcount</name>
    <direction>Output</direction>
    <width>5</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dts_slave_waitrequest</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dts_slave_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>pcie_256_hip_avmm_0</moduleName>
    <slaveName>rd_dts_slave</slaveName>
    <name>pcie_256_hip_avmm_0.rd_dts_slave</name>
    <baseAddress>0</baseAddress>
    <span>8192</span>
   </memoryBlock>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_wr_dts_slave"
     kind="avalon_master"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>onchip_memory2_0_reset1_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dts_slave_address</name>
    <direction>Output</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dts_slave_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dts_slave_writedata</name>
    <direction>Output</direction>
    <width>256</width>
    <role>writedata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dts_slave_burstcount</name>
    <direction>Output</direction>
    <width>5</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dts_slave_waitrequest</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dts_slave_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>pcie_256_hip_avmm_0</moduleName>
    <slaveName>wr_dts_slave</slaveName>
    <name>pcie_256_hip_avmm_0.wr_dts_slave</name>
    <baseAddress>0</baseAddress>
    <span>8192</span>
   </memoryBlock>
  </interface>
 </module>
 <module
   name="mm_interconnect_2"
   kind="altera_mm_interconnect"
   version="14.0"
   path="mm_interconnect_2">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>interconnect_id.onchip_memory2_0.s2</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.dma_wr_master</name>
   <value>0</value>
  </assignment>
  <parameter name="COMPOSE_CONTENTS">
   <type>java.lang.String</type>
   <value><![CDATA[add_instance {pcie_256_hip_avmm_0_dma_wr_master_translator} {altera_merlin_master_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_DATA_W} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_BURSTCOUNT_W} {6};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_BYTEENABLE_W} {16};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {UAV_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_READDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_WRITEDATA} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_READ} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_WRITE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_BYTEENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_BURSTCOUNT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_READDATAVALID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_SYMBOLS_PER_WORD} {16};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_CONSTANT_BURST_BEHAVIOR} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator} {AV_ALWAYSBURSTMAXBURST} {0};add_instance {onchip_memory2_0_s2_translator} {altera_merlin_slave_translator};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_ADDRESS_W} {8};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_DATA_W} {128};set_instance_parameter_value {onchip_memory2_0_s2_translator} {UAV_DATA_W} {128};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_BYTEENABLE_W} {16};set_instance_parameter_value {onchip_memory2_0_s2_translator} {UAV_BYTEENABLE_W} {16};set_instance_parameter_value {onchip_memory2_0_s2_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {onchip_memory2_0_s2_translator} {UAV_BURSTCOUNT_W} {5};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_READLATENCY} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_READ_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_READDATA} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_READ} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_WRITE} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_ADDRESS} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_WAITREQUEST} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_LOCK} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_AV_CLKEN} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_SYMBOLS_PER_WORD} {16};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {onchip_memory2_0_s2_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {pcie_256_hip_avmm_0_dma_wr_master_agent} {altera_merlin_master_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_PROTECTION_H} {239};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_PROTECTION_L} {237};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BEGIN_BURST} {232};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BURSTWRAP_H} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BURSTWRAP_L} {224};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BURST_SIZE_H} {227};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BURST_SIZE_L} {225};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BURST_TYPE_H} {229};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BURST_TYPE_L} {228};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BYTE_CNT_H} {223};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BYTE_CNT_L} {214};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_ADDR_H} {207};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_ADDR_L} {144};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_TRANS_POSTED} {209};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_TRANS_READ} {211};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_TRANS_EXCLUSIVE} {213};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_DATA_H} {127};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BYTEEN_H} {143};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_BYTEEN_L} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_SRC_ID_H} {234};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_SRC_ID_L} {234};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_DEST_ID_H} {235};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_DEST_ID_L} {235};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_THREAD_ID_H} {236};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_THREAD_ID_L} {236};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_CACHE_H} {243};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_CACHE_L} {240};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_DATA_SIDEBAND_H} {231};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_DATA_SIDEBAND_L} {231};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_QOS_H} {233};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_QOS_L} {233};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_ADDR_SIDEBAND_H} {230};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_ADDR_SIDEBAND_L} {230};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_RESPONSE_STATUS_H} {245};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_RESPONSE_STATUS_L} {244};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_ORI_BURST_SIZE_L} {246};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {PKT_ORI_BURST_SIZE_H} {248};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {ST_DATA_W} {249};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {ST_CHANNEL_W} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {AV_BURSTCOUNT_W} {10};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {ADDR_MAP} {<?xml version="1.0" encoding="UTF-8"?>
<address_map>
 <slave
   id="0"
   name="onchip_memory2_0_s2_translator.avalon_universal_slave_0"
   start="0x0000000000000000"
   end="0x00000000000001000"
   responds="1"
   user_default="0" />
</address_map>
};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {SUPPRESS_0_BYTEEN_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {ID} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {BURSTWRAP_VALUE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {CACHE_VALUE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {SECURE_ACCESS_BIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_agent} {USE_WRITERESPONSE} {0};add_instance {onchip_memory2_0_s2_agent} {altera_merlin_slave_agent};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_DATA_H} {127};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_DATA_L} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BEGIN_BURST} {232};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BYTEEN_H} {143};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BYTEEN_L} {128};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_ADDR_H} {207};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_ADDR_L} {144};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_TRANS_POSTED} {209};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_TRANS_READ} {211};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_SRC_ID_H} {234};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_SRC_ID_L} {234};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_DEST_ID_H} {235};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_DEST_ID_L} {235};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BURSTWRAP_H} {224};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BURSTWRAP_L} {224};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BYTE_CNT_H} {223};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BYTE_CNT_L} {214};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_PROTECTION_H} {239};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_PROTECTION_L} {237};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_RESPONSE_STATUS_H} {245};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_RESPONSE_STATUS_L} {244};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BURST_SIZE_H} {227};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_BURST_SIZE_L} {225};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_ORI_BURST_SIZE_L} {246};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PKT_ORI_BURST_SIZE_H} {248};set_instance_parameter_value {onchip_memory2_0_s2_agent} {ST_CHANNEL_W} {1};set_instance_parameter_value {onchip_memory2_0_s2_agent} {ST_DATA_W} {249};set_instance_parameter_value {onchip_memory2_0_s2_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent} {AVS_BURSTCOUNT_W} {5};set_instance_parameter_value {onchip_memory2_0_s2_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {onchip_memory2_0_s2_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {onchip_memory2_0_s2_agent} {MAX_BYTE_CNT} {16};set_instance_parameter_value {onchip_memory2_0_s2_agent} {MAX_BURSTWRAP} {1};set_instance_parameter_value {onchip_memory2_0_s2_agent} {ID} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent} {USE_WRITERESPONSE} {0};add_instance {onchip_memory2_0_s2_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {BITS_PER_SYMBOL} {250};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {onchip_memory2_0_s2_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {router} {altera_merlin_router};set_instance_parameter_value {router} {DESTINATION_ID} {0 };set_instance_parameter_value {router} {CHANNEL_ID} {1 };set_instance_parameter_value {router} {TYPE_OF_TRANSACTION} {both };set_instance_parameter_value {router} {START_ADDRESS} {0x0 };set_instance_parameter_value {router} {END_ADDRESS} {0x1000 };set_instance_parameter_value {router} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router} {SPAN_OFFSET} {};set_instance_parameter_value {router} {PKT_ADDR_H} {207};set_instance_parameter_value {router} {PKT_ADDR_L} {144};set_instance_parameter_value {router} {PKT_PROTECTION_H} {239};set_instance_parameter_value {router} {PKT_PROTECTION_L} {237};set_instance_parameter_value {router} {PKT_DEST_ID_H} {235};set_instance_parameter_value {router} {PKT_DEST_ID_L} {235};set_instance_parameter_value {router} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {router} {PKT_TRANS_READ} {211};set_instance_parameter_value {router} {ST_DATA_W} {249};set_instance_parameter_value {router} {ST_CHANNEL_W} {1};set_instance_parameter_value {router} {DECODER_TYPE} {0};set_instance_parameter_value {router} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_DESTID} {0};set_instance_parameter_value {router} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {router} {MEMORY_ALIASING_DECODE} {0};add_instance {router_001} {altera_merlin_router};set_instance_parameter_value {router_001} {DESTINATION_ID} {0 };set_instance_parameter_value {router_001} {CHANNEL_ID} {1 };set_instance_parameter_value {router_001} {TYPE_OF_TRANSACTION} {read };set_instance_parameter_value {router_001} {START_ADDRESS} {0x0 };set_instance_parameter_value {router_001} {END_ADDRESS} {0x0 };set_instance_parameter_value {router_001} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router_001} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router_001} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router_001} {SPAN_OFFSET} {};set_instance_parameter_value {router_001} {PKT_ADDR_H} {207};set_instance_parameter_value {router_001} {PKT_ADDR_L} {144};set_instance_parameter_value {router_001} {PKT_PROTECTION_H} {239};set_instance_parameter_value {router_001} {PKT_PROTECTION_L} {237};set_instance_parameter_value {router_001} {PKT_DEST_ID_H} {235};set_instance_parameter_value {router_001} {PKT_DEST_ID_L} {235};set_instance_parameter_value {router_001} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {router_001} {PKT_TRANS_READ} {211};set_instance_parameter_value {router_001} {ST_DATA_W} {249};set_instance_parameter_value {router_001} {ST_CHANNEL_W} {1};set_instance_parameter_value {router_001} {DECODER_TYPE} {1};set_instance_parameter_value {router_001} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_001} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {router_001} {MEMORY_ALIASING_DECODE} {0};add_instance {onchip_memory2_0_s2_burst_adapter} {altera_merlin_burst_adapter};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_ADDR_H} {207};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_ADDR_L} {144};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BEGIN_BURST} {232};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BYTE_CNT_H} {223};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BYTE_CNT_L} {214};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BYTEEN_H} {143};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BYTEEN_L} {128};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BURST_SIZE_H} {227};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BURST_SIZE_L} {225};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BURST_TYPE_H} {229};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BURST_TYPE_L} {228};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BURSTWRAP_H} {224};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_BURSTWRAP_L} {224};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_TRANS_COMPRESSED_READ} {208};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_TRANS_WRITE} {210};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PKT_TRANS_READ} {211};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {OUT_NARROW_SIZE} {0};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {IN_NARROW_SIZE} {0};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {OUT_FIXED} {0};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {OUT_COMPLETE_WRAP} {0};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {ST_DATA_W} {249};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {ST_CHANNEL_W} {1};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {OUT_BYTE_CNT_H} {218};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {OUT_BURSTWRAP_H} {224};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {COMPRESSED_READ_SUPPORT} {1};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {BYTEENABLE_SYNTHESIS} {1};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {PIPE_INPUTS} {0};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {NO_WRAP_SUPPORT} {0};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {INCOMPLETE_WRAP_SUPPORT} {0};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {BURSTWRAP_CONST_MASK} {1};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {BURSTWRAP_CONST_VALUE} {1};set_instance_parameter_value {onchip_memory2_0_s2_burst_adapter} {ADAPTER_VERSION} {13.1};add_instance {cmd_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {cmd_demux} {ST_DATA_W} {249};set_instance_parameter_value {cmd_demux} {ST_CHANNEL_W} {1};set_instance_parameter_value {cmd_demux} {NUM_OUTPUTS} {1};set_instance_parameter_value {cmd_demux} {VALID_WIDTH} {1};set_instance_parameter_value {cmd_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {cmd_mux} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux} {ST_DATA_W} {249};set_instance_parameter_value {cmd_mux} {ST_CHANNEL_W} {1};set_instance_parameter_value {cmd_mux} {NUM_INPUTS} {1};set_instance_parameter_value {cmd_mux} {PIPELINE_ARB} {0};set_instance_parameter_value {cmd_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {cmd_mux} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {cmd_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {rsp_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux} {ST_DATA_W} {249};set_instance_parameter_value {rsp_demux} {ST_CHANNEL_W} {1};set_instance_parameter_value {rsp_demux} {NUM_OUTPUTS} {1};set_instance_parameter_value {rsp_demux} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {rsp_mux} {altera_merlin_multiplexer};set_instance_parameter_value {rsp_mux} {ST_DATA_W} {249};set_instance_parameter_value {rsp_mux} {ST_CHANNEL_W} {1};set_instance_parameter_value {rsp_mux} {NUM_INPUTS} {1};set_instance_parameter_value {rsp_mux} {PIPELINE_ARB} {0};set_instance_parameter_value {rsp_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {rsp_mux} {PKT_TRANS_LOCK} {212};set_instance_parameter_value {rsp_mux} {ARBITRATION_SCHEME} {no-arb};set_instance_parameter_value {rsp_mux} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {rsp_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(248:246) response_status(245:244) cache(243:240) protection(239:237) thread_id(236) dest_id(235) src_id(234) qos(233) begin_burst(232) data_sideband(231) addr_sideband(230) burst_type(229:228) burst_size(227:225) burstwrap(224) byte_cnt(223:214) trans_exclusive(213) trans_lock(212) trans_read(211) trans_write(210) trans_posted(209) trans_compressed_read(208) addr(207:144) byteen(143:128) data(127:0)};add_instance {onchip_memory2_0_reset2_reset_bridge} {altera_reset_bridge};set_instance_parameter_value {onchip_memory2_0_reset2_reset_bridge} {ACTIVE_LOW_RESET} {0};set_instance_parameter_value {onchip_memory2_0_reset2_reset_bridge} {SYNCHRONOUS_EDGES} {deassert};set_instance_parameter_value {onchip_memory2_0_reset2_reset_bridge} {NUM_RESET_OUTPUTS} {1};add_instance {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {altera_clock_bridge};set_instance_parameter_value {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {EXPLICIT_CLOCK_RATE} {125000000};set_instance_parameter_value {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {NUM_CLOCK_OUTPUTS} {1};add_connection {pcie_256_hip_avmm_0_dma_wr_master_translator.avalon_universal_master_0} {pcie_256_hip_avmm_0_dma_wr_master_agent.av} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_dma_wr_master_agent.av} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_dma_wr_master_agent.av} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_dma_wr_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_dma_wr_master_agent.av} {defaultConnection} {false};add_connection {rsp_mux.src} {pcie_256_hip_avmm_0_dma_wr_master_agent.rp} {avalon_streaming};preview_set_connection_tag {rsp_mux.src/pcie_256_hip_avmm_0_dma_wr_master_agent.rp} {qsys_mm.response};add_connection {onchip_memory2_0_s2_agent.m0} {onchip_memory2_0_s2_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {onchip_memory2_0_s2_agent.m0/onchip_memory2_0_s2_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {onchip_memory2_0_s2_agent.m0/onchip_memory2_0_s2_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {onchip_memory2_0_s2_agent.m0/onchip_memory2_0_s2_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {onchip_memory2_0_s2_agent.rf_source} {onchip_memory2_0_s2_agent_rsp_fifo.in} {avalon_streaming};add_connection {onchip_memory2_0_s2_agent_rsp_fifo.out} {onchip_memory2_0_s2_agent.rf_sink} {avalon_streaming};add_connection {onchip_memory2_0_s2_agent.rdata_fifo_src} {onchip_memory2_0_s2_agent.rdata_fifo_sink} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_dma_wr_master_agent.cp} {router.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_dma_wr_master_agent.cp/router.sink} {qsys_mm.command};add_connection {router.src} {cmd_demux.sink} {avalon_streaming};preview_set_connection_tag {router.src/cmd_demux.sink} {qsys_mm.command};add_connection {onchip_memory2_0_s2_agent.rp} {router_001.sink} {avalon_streaming};preview_set_connection_tag {onchip_memory2_0_s2_agent.rp/router_001.sink} {qsys_mm.response};add_connection {router_001.src} {rsp_demux.sink} {avalon_streaming};preview_set_connection_tag {router_001.src/rsp_demux.sink} {qsys_mm.response};add_connection {cmd_mux.src} {onchip_memory2_0_s2_burst_adapter.sink0} {avalon_streaming};preview_set_connection_tag {cmd_mux.src/onchip_memory2_0_s2_burst_adapter.sink0} {qsys_mm.command};add_connection {onchip_memory2_0_s2_burst_adapter.source0} {onchip_memory2_0_s2_agent.cp} {avalon_streaming};preview_set_connection_tag {onchip_memory2_0_s2_burst_adapter.source0/onchip_memory2_0_s2_agent.cp} {qsys_mm.command};add_connection {cmd_demux.src0} {cmd_mux.sink0} {avalon_streaming};preview_set_connection_tag {cmd_demux.src0/cmd_mux.sink0} {qsys_mm.command};add_connection {rsp_demux.src0} {rsp_mux.sink0} {avalon_streaming};preview_set_connection_tag {rsp_demux.src0/rsp_mux.sink0} {qsys_mm.response};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {pcie_256_hip_avmm_0_dma_wr_master_translator.reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {onchip_memory2_0_s2_translator.reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {pcie_256_hip_avmm_0_dma_wr_master_agent.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {onchip_memory2_0_s2_agent.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {onchip_memory2_0_s2_agent_rsp_fifo.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {router.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {router_001.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {onchip_memory2_0_s2_burst_adapter.cr0_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {cmd_demux.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {cmd_mux.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {rsp_demux.clk_reset} {reset};add_connection {onchip_memory2_0_reset2_reset_bridge.out_reset} {rsp_mux.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_dma_wr_master_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s2_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_dma_wr_master_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s2_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s2_agent_rsp_fifo.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_s2_burst_adapter.cr0} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_demux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_mux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_mux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_demux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {onchip_memory2_0_reset2_reset_bridge.clk} {clock};add_interface {pcie_256_hip_avmm_0_coreclkout} {clock} {slave};set_interface_property {pcie_256_hip_avmm_0_coreclkout} {EXPORT_OF} {pcie_256_hip_avmm_0_coreclkout_clock_bridge.in_clk};add_interface {onchip_memory2_0_reset2_reset_bridge_in_reset} {reset} {slave};set_interface_property {onchip_memory2_0_reset2_reset_bridge_in_reset} {EXPORT_OF} {onchip_memory2_0_reset2_reset_bridge.in_reset};add_interface {pcie_256_hip_avmm_0_dma_wr_master} {avalon} {slave};set_interface_property {pcie_256_hip_avmm_0_dma_wr_master} {EXPORT_OF} {pcie_256_hip_avmm_0_dma_wr_master_translator.avalon_anti_master_0};add_interface {onchip_memory2_0_s2} {avalon} {master};set_interface_property {onchip_memory2_0_s2} {EXPORT_OF} {onchip_memory2_0_s2_translator.avalon_anti_slave_0};set_module_assignment {interconnect_id.onchip_memory2_0.s2} {0};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.dma_wr_master} {0};]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_DEVICE_FAMILY">
   <type>java.lang.String</type>
   <value>ARRIAV</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="AUTO_DEVICE">
   <type>java.lang.String</type>
   <value>5AGXFB3H4F35C5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE</sysinfo_type>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>Arria V</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface
     name="pcie_256_hip_avmm_0_coreclkout"
     kind="clock_sink"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_coreclkout_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface
     name="onchip_memory2_0_reset2_reset_bridge_in_reset"
     kind="reset_sink"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>onchip_memory2_0_reset2_reset_bridge_in_reset_reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_dma_wr_master"
     kind="avalon_slave"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>merlin.flow.avalon_universal_master_0</name>
    <value>avalon_universal_master_0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>18446744073709551616</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>onchip_memory2_0_reset2_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_dma_wr_master_address</name>
    <direction>Input</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_wr_master_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_wr_master_burstcount</name>
    <direction>Input</direction>
    <width>6</width>
    <role>burstcount</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_wr_master_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_wr_master_readdata</name>
    <direction>Output</direction>
    <width>128</width>
    <role>readdata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_dma_wr_master_readdatavalid</name>
    <direction>Output</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
  </interface>
  <interface name="onchip_memory2_0_s2" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>onchip_memory2_0_reset2_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>onchip_memory2_0_s2_address</name>
    <direction>Output</direction>
    <width>8</width>
    <role>address</role>
   </port>
   <port>
    <name>onchip_memory2_0_s2_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>onchip_memory2_0_s2_readdata</name>
    <direction>Input</direction>
    <width>128</width>
    <role>readdata</role>
   </port>
   <port>
    <name>onchip_memory2_0_s2_writedata</name>
    <direction>Output</direction>
    <width>128</width>
    <role>writedata</role>
   </port>
   <port>
    <name>onchip_memory2_0_s2_byteenable</name>
    <direction>Output</direction>
    <width>16</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>onchip_memory2_0_s2_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>onchip_memory2_0_s2_clken</name>
    <direction>Output</direction>
    <width>1</width>
    <role>clken</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>onchip_memory2_0</moduleName>
    <slaveName>s2</slaveName>
    <name>onchip_memory2_0.s2</name>
    <baseAddress>0</baseAddress>
    <span>4096</span>
   </memoryBlock>
  </interface>
 </module>
 <module
   name="mm_interconnect_3"
   kind="altera_mm_interconnect"
   version="14.0"
   path="mm_interconnect_3">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.Txs</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.rd_dcm_master</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pcie_256_hip_avmm_0.wr_dcm_master</name>
   <value>1</value>
  </assignment>
  <parameter name="COMPOSE_CONTENTS">
   <type>java.lang.String</type>
   <value><![CDATA[add_instance {pcie_256_hip_avmm_0_wr_dcm_master_translator} {altera_merlin_master_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_DATA_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_READDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_READ} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_WRITE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_READDATAVALID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator} {AV_ALWAYSBURSTMAXBURST} {0};add_instance {pcie_256_hip_avmm_0_rd_dcm_master_translator} {altera_merlin_master_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_DATA_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_READDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_READ} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_WRITE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_READDATAVALID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator} {AV_ALWAYSBURSTMAXBURST} {0};add_instance {pcie_256_hip_avmm_0_Txs_translator} {altera_merlin_slave_translator};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_ADDRESS_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_DATA_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {UAV_DATA_W} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {UAV_BYTEENABLE_W} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {UAV_ADDRESS_W} {64};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_WRITE_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_READDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_READ} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_WRITE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_READDATAVALID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_LOCK} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_AV_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {pcie_256_hip_avmm_0_wr_dcm_master_agent} {altera_merlin_master_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_PROTECTION_H} {124};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_PROTECTION_L} {122};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BEGIN_BURST} {117};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BURSTWRAP_H} {109};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BURSTWRAP_L} {109};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BURST_SIZE_H} {112};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BURST_SIZE_L} {110};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BURST_TYPE_H} {114};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BURST_TYPE_L} {113};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BYTE_CNT_H} {108};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BYTE_CNT_L} {106};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_ADDR_H} {99};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_TRANS_COMPRESSED_READ} {100};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_TRANS_POSTED} {101};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_TRANS_READ} {103};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_TRANS_EXCLUSIVE} {105};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_DATA_H} {31};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_SRC_ID_H} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_SRC_ID_L} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_DEST_ID_H} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_DEST_ID_L} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_THREAD_ID_H} {121};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_THREAD_ID_L} {121};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_CACHE_H} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_CACHE_L} {125};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_DATA_SIDEBAND_H} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_DATA_SIDEBAND_L} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_QOS_H} {118};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_QOS_L} {118};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_ADDR_SIDEBAND_H} {115};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_ADDR_SIDEBAND_L} {115};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_RESPONSE_STATUS_H} {130};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_RESPONSE_STATUS_L} {129};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_ORI_BURST_SIZE_L} {131};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {PKT_ORI_BURST_SIZE_H} {133};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {ST_DATA_W} {134};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {ST_CHANNEL_W} {2};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {AV_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {ADDR_MAP} {<?xml version="1.0" encoding="UTF-8"?>
<address_map>
 <slave
   id="0"
   name="pcie_256_hip_avmm_0_Txs_translator.avalon_universal_slave_0"
   start="0x0000000000000000"
   end="0x00000000100000000"
   responds="1"
   user_default="0" />
</address_map>
};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {SUPPRESS_0_BYTEEN_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {ID} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {BURSTWRAP_VALUE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {CACHE_VALUE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {SECURE_ACCESS_BIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_agent} {USE_WRITERESPONSE} {0};add_instance {pcie_256_hip_avmm_0_rd_dcm_master_agent} {altera_merlin_master_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_PROTECTION_H} {124};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_PROTECTION_L} {122};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BEGIN_BURST} {117};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BURSTWRAP_H} {109};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BURSTWRAP_L} {109};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BURST_SIZE_H} {112};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BURST_SIZE_L} {110};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BURST_TYPE_H} {114};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BURST_TYPE_L} {113};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BYTE_CNT_H} {108};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BYTE_CNT_L} {106};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_ADDR_H} {99};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_TRANS_COMPRESSED_READ} {100};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_TRANS_POSTED} {101};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_TRANS_READ} {103};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_TRANS_EXCLUSIVE} {105};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_DATA_H} {31};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_SRC_ID_H} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_SRC_ID_L} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_DEST_ID_H} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_DEST_ID_L} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_THREAD_ID_H} {121};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_THREAD_ID_L} {121};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_CACHE_H} {128};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_CACHE_L} {125};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_DATA_SIDEBAND_H} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_DATA_SIDEBAND_L} {116};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_QOS_H} {118};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_QOS_L} {118};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_ADDR_SIDEBAND_H} {115};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_ADDR_SIDEBAND_L} {115};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_RESPONSE_STATUS_H} {130};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_RESPONSE_STATUS_L} {129};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_ORI_BURST_SIZE_L} {131};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {PKT_ORI_BURST_SIZE_H} {133};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {ST_DATA_W} {134};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {ST_CHANNEL_W} {2};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {AV_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {ADDR_MAP} {<?xml version="1.0" encoding="UTF-8"?>
<address_map>
 <slave
   id="0"
   name="pcie_256_hip_avmm_0_Txs_translator.avalon_universal_slave_0"
   start="0x0000000000000000"
   end="0x00000000100000000"
   responds="1"
   user_default="0" />
</address_map>
};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {SUPPRESS_0_BYTEEN_RSP} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {ID} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {BURSTWRAP_VALUE} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {CACHE_VALUE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {SECURE_ACCESS_BIT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_agent} {USE_WRITERESPONSE} {0};add_instance {pcie_256_hip_avmm_0_Txs_agent} {altera_merlin_slave_agent};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_DATA_H} {31};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BEGIN_BURST} {117};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_ADDR_H} {99};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_TRANS_COMPRESSED_READ} {100};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_TRANS_POSTED} {101};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_TRANS_READ} {103};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_SRC_ID_H} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_SRC_ID_L} {119};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_DEST_ID_H} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_DEST_ID_L} {120};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BURSTWRAP_H} {109};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BURSTWRAP_L} {109};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BYTE_CNT_H} {108};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BYTE_CNT_L} {106};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_PROTECTION_H} {124};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_PROTECTION_L} {122};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_RESPONSE_STATUS_H} {130};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_RESPONSE_STATUS_L} {129};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BURST_SIZE_H} {112};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_BURST_SIZE_L} {110};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_ORI_BURST_SIZE_L} {131};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PKT_ORI_BURST_SIZE_H} {133};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {ST_CHANNEL_W} {2};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {ST_DATA_W} {134};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {AVS_BURSTCOUNT_W} {3};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {MAX_BYTE_CNT} {4};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {MAX_BURSTWRAP} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {ID} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent} {USE_WRITERESPONSE} {0};add_instance {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {BITS_PER_SYMBOL} {135};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {FIFO_DEPTH} {9};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {router} {altera_merlin_router};set_instance_parameter_value {router} {DESTINATION_ID} {0 };set_instance_parameter_value {router} {CHANNEL_ID} {1 };set_instance_parameter_value {router} {TYPE_OF_TRANSACTION} {both };set_instance_parameter_value {router} {START_ADDRESS} {0x0 };set_instance_parameter_value {router} {END_ADDRESS} {0x100000000 };set_instance_parameter_value {router} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router} {SPAN_OFFSET} {};set_instance_parameter_value {router} {PKT_ADDR_H} {99};set_instance_parameter_value {router} {PKT_ADDR_L} {36};set_instance_parameter_value {router} {PKT_PROTECTION_H} {124};set_instance_parameter_value {router} {PKT_PROTECTION_L} {122};set_instance_parameter_value {router} {PKT_DEST_ID_H} {120};set_instance_parameter_value {router} {PKT_DEST_ID_L} {120};set_instance_parameter_value {router} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {router} {PKT_TRANS_READ} {103};set_instance_parameter_value {router} {ST_DATA_W} {134};set_instance_parameter_value {router} {ST_CHANNEL_W} {2};set_instance_parameter_value {router} {DECODER_TYPE} {0};set_instance_parameter_value {router} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_DESTID} {0};set_instance_parameter_value {router} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router} {MEMORY_ALIASING_DECODE} {0};add_instance {router_001} {altera_merlin_router};set_instance_parameter_value {router_001} {DESTINATION_ID} {0 };set_instance_parameter_value {router_001} {CHANNEL_ID} {1 };set_instance_parameter_value {router_001} {TYPE_OF_TRANSACTION} {both };set_instance_parameter_value {router_001} {START_ADDRESS} {0x0 };set_instance_parameter_value {router_001} {END_ADDRESS} {0x100000000 };set_instance_parameter_value {router_001} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router_001} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router_001} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router_001} {SPAN_OFFSET} {};set_instance_parameter_value {router_001} {PKT_ADDR_H} {99};set_instance_parameter_value {router_001} {PKT_ADDR_L} {36};set_instance_parameter_value {router_001} {PKT_PROTECTION_H} {124};set_instance_parameter_value {router_001} {PKT_PROTECTION_L} {122};set_instance_parameter_value {router_001} {PKT_DEST_ID_H} {120};set_instance_parameter_value {router_001} {PKT_DEST_ID_L} {120};set_instance_parameter_value {router_001} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {router_001} {PKT_TRANS_READ} {103};set_instance_parameter_value {router_001} {ST_DATA_W} {134};set_instance_parameter_value {router_001} {ST_CHANNEL_W} {2};set_instance_parameter_value {router_001} {DECODER_TYPE} {0};set_instance_parameter_value {router_001} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_001} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router_001} {MEMORY_ALIASING_DECODE} {0};add_instance {router_002} {altera_merlin_router};set_instance_parameter_value {router_002} {DESTINATION_ID} {1 0 };set_instance_parameter_value {router_002} {CHANNEL_ID} {01 10 };set_instance_parameter_value {router_002} {TYPE_OF_TRANSACTION} {both both };set_instance_parameter_value {router_002} {START_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_002} {END_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_002} {NON_SECURED_TAG} {1 1 };set_instance_parameter_value {router_002} {SECURED_RANGE_PAIRS} {0 0 };set_instance_parameter_value {router_002} {SECURED_RANGE_LIST} {0 0 };set_instance_parameter_value {router_002} {SPAN_OFFSET} {};set_instance_parameter_value {router_002} {PKT_ADDR_H} {99};set_instance_parameter_value {router_002} {PKT_ADDR_L} {36};set_instance_parameter_value {router_002} {PKT_PROTECTION_H} {124};set_instance_parameter_value {router_002} {PKT_PROTECTION_L} {122};set_instance_parameter_value {router_002} {PKT_DEST_ID_H} {120};set_instance_parameter_value {router_002} {PKT_DEST_ID_L} {120};set_instance_parameter_value {router_002} {PKT_TRANS_WRITE} {102};set_instance_parameter_value {router_002} {PKT_TRANS_READ} {103};set_instance_parameter_value {router_002} {ST_DATA_W} {134};set_instance_parameter_value {router_002} {ST_CHANNEL_W} {2};set_instance_parameter_value {router_002} {DECODER_TYPE} {1};set_instance_parameter_value {router_002} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_002} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_002} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_002} {DEFAULT_DESTID} {1};set_instance_parameter_value {router_002} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router_002} {MEMORY_ALIASING_DECODE} {0};add_instance {cmd_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {cmd_demux} {ST_DATA_W} {134};set_instance_parameter_value {cmd_demux} {ST_CHANNEL_W} {2};set_instance_parameter_value {cmd_demux} {NUM_OUTPUTS} {1};set_instance_parameter_value {cmd_demux} {VALID_WIDTH} {1};set_instance_parameter_value {cmd_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {cmd_demux_001} {altera_merlin_demultiplexer};set_instance_parameter_value {cmd_demux_001} {ST_DATA_W} {134};set_instance_parameter_value {cmd_demux_001} {ST_CHANNEL_W} {2};set_instance_parameter_value {cmd_demux_001} {NUM_OUTPUTS} {1};set_instance_parameter_value {cmd_demux_001} {VALID_WIDTH} {1};set_instance_parameter_value {cmd_demux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {cmd_mux} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux} {ST_DATA_W} {134};set_instance_parameter_value {cmd_mux} {ST_CHANNEL_W} {2};set_instance_parameter_value {cmd_mux} {NUM_INPUTS} {2};set_instance_parameter_value {cmd_mux} {PIPELINE_ARB} {0};set_instance_parameter_value {cmd_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {cmd_mux} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux} {ARBITRATION_SHARES} {1 1 };set_instance_parameter_value {cmd_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {rsp_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux} {ST_DATA_W} {134};set_instance_parameter_value {rsp_demux} {ST_CHANNEL_W} {2};set_instance_parameter_value {rsp_demux} {NUM_OUTPUTS} {2};set_instance_parameter_value {rsp_demux} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {rsp_mux} {altera_merlin_multiplexer};set_instance_parameter_value {rsp_mux} {ST_DATA_W} {134};set_instance_parameter_value {rsp_mux} {ST_CHANNEL_W} {2};set_instance_parameter_value {rsp_mux} {NUM_INPUTS} {1};set_instance_parameter_value {rsp_mux} {PIPELINE_ARB} {0};set_instance_parameter_value {rsp_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {rsp_mux} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {rsp_mux} {ARBITRATION_SCHEME} {no-arb};set_instance_parameter_value {rsp_mux} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {rsp_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {rsp_mux_001} {altera_merlin_multiplexer};set_instance_parameter_value {rsp_mux_001} {ST_DATA_W} {134};set_instance_parameter_value {rsp_mux_001} {ST_CHANNEL_W} {2};set_instance_parameter_value {rsp_mux_001} {NUM_INPUTS} {1};set_instance_parameter_value {rsp_mux_001} {PIPELINE_ARB} {0};set_instance_parameter_value {rsp_mux_001} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {rsp_mux_001} {PKT_TRANS_LOCK} {104};set_instance_parameter_value {rsp_mux_001} {ARBITRATION_SCHEME} {no-arb};set_instance_parameter_value {rsp_mux_001} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {rsp_mux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(133:131) response_status(130:129) cache(128:125) protection(124:122) thread_id(121) dest_id(120) src_id(119) qos(118) begin_burst(117) data_sideband(116) addr_sideband(115) burst_type(114:113) burst_size(112:110) burstwrap(109) byte_cnt(108:106) trans_exclusive(105) trans_lock(104) trans_read(103) trans_write(102) trans_posted(101) trans_compressed_read(100) addr(99:36) byteen(35:32) data(31:0)};add_instance {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge} {altera_reset_bridge};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge} {ACTIVE_LOW_RESET} {0};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge} {SYNCHRONOUS_EDGES} {deassert};set_instance_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge} {NUM_RESET_OUTPUTS} {1};add_instance {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {altera_clock_bridge};set_instance_parameter_value {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {EXPLICIT_CLOCK_RATE} {125000000};set_instance_parameter_value {pcie_256_hip_avmm_0_coreclkout_clock_bridge} {NUM_CLOCK_OUTPUTS} {1};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator.avalon_universal_master_0} {pcie_256_hip_avmm_0_wr_dcm_master_agent.av} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_wr_dcm_master_agent.av} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_wr_dcm_master_agent.av} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_wr_dcm_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_wr_dcm_master_agent.av} {defaultConnection} {false};add_connection {rsp_mux.src} {pcie_256_hip_avmm_0_wr_dcm_master_agent.rp} {avalon_streaming};preview_set_connection_tag {rsp_mux.src/pcie_256_hip_avmm_0_wr_dcm_master_agent.rp} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_rd_dcm_master_translator.avalon_universal_master_0} {pcie_256_hip_avmm_0_rd_dcm_master_agent.av} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_rd_dcm_master_agent.av} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_rd_dcm_master_agent.av} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_rd_dcm_master_translator.avalon_universal_master_0/pcie_256_hip_avmm_0_rd_dcm_master_agent.av} {defaultConnection} {false};add_connection {rsp_mux_001.src} {pcie_256_hip_avmm_0_rd_dcm_master_agent.rp} {avalon_streaming};preview_set_connection_tag {rsp_mux_001.src/pcie_256_hip_avmm_0_rd_dcm_master_agent.rp} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_Txs_agent.m0} {pcie_256_hip_avmm_0_Txs_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {pcie_256_hip_avmm_0_Txs_agent.m0/pcie_256_hip_avmm_0_Txs_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {pcie_256_hip_avmm_0_Txs_agent.m0/pcie_256_hip_avmm_0_Txs_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {pcie_256_hip_avmm_0_Txs_agent.m0/pcie_256_hip_avmm_0_Txs_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {pcie_256_hip_avmm_0_Txs_agent.rf_source} {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo.in} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo.out} {pcie_256_hip_avmm_0_Txs_agent.rf_sink} {avalon_streaming};add_connection {pcie_256_hip_avmm_0_Txs_agent.rdata_fifo_src} {pcie_256_hip_avmm_0_Txs_agent.rdata_fifo_sink} {avalon_streaming};add_connection {cmd_mux.src} {pcie_256_hip_avmm_0_Txs_agent.cp} {avalon_streaming};preview_set_connection_tag {cmd_mux.src/pcie_256_hip_avmm_0_Txs_agent.cp} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_agent.cp} {router.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_wr_dcm_master_agent.cp/router.sink} {qsys_mm.command};add_connection {router.src} {cmd_demux.sink} {avalon_streaming};preview_set_connection_tag {router.src/cmd_demux.sink} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_rd_dcm_master_agent.cp} {router_001.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_rd_dcm_master_agent.cp/router_001.sink} {qsys_mm.command};add_connection {router_001.src} {cmd_demux_001.sink} {avalon_streaming};preview_set_connection_tag {router_001.src/cmd_demux_001.sink} {qsys_mm.command};add_connection {pcie_256_hip_avmm_0_Txs_agent.rp} {router_002.sink} {avalon_streaming};preview_set_connection_tag {pcie_256_hip_avmm_0_Txs_agent.rp/router_002.sink} {qsys_mm.response};add_connection {router_002.src} {rsp_demux.sink} {avalon_streaming};preview_set_connection_tag {router_002.src/rsp_demux.sink} {qsys_mm.response};add_connection {cmd_demux.src0} {cmd_mux.sink0} {avalon_streaming};preview_set_connection_tag {cmd_demux.src0/cmd_mux.sink0} {qsys_mm.command};add_connection {cmd_demux_001.src0} {cmd_mux.sink1} {avalon_streaming};preview_set_connection_tag {cmd_demux_001.src0/cmd_mux.sink1} {qsys_mm.command};add_connection {rsp_demux.src0} {rsp_mux.sink0} {avalon_streaming};preview_set_connection_tag {rsp_demux.src0/rsp_mux.sink0} {qsys_mm.response};add_connection {rsp_demux.src1} {rsp_mux_001.sink0} {avalon_streaming};preview_set_connection_tag {rsp_demux.src1/rsp_mux_001.sink0} {qsys_mm.response};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dcm_master_translator.reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dcm_master_translator.reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {pcie_256_hip_avmm_0_Txs_translator.reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {pcie_256_hip_avmm_0_wr_dcm_master_agent.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {pcie_256_hip_avmm_0_rd_dcm_master_agent.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {pcie_256_hip_avmm_0_Txs_agent.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {router.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {router_001.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {router_002.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {cmd_demux.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {cmd_demux_001.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {cmd_mux.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {rsp_demux.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {rsp_mux.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.out_reset} {rsp_mux_001.clk_reset} {reset};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dcm_master_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dcm_master_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_Txs_translator.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dcm_master_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_rd_dcm_master_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_Txs_agent.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_Txs_agent_rsp_fifo.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {router_002.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_demux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_mux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_demux_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_mux_001.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {cmd_mux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {rsp_demux.clk} {clock};add_connection {pcie_256_hip_avmm_0_coreclkout_clock_bridge.out_clk} {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.clk} {clock};add_interface {pcie_256_hip_avmm_0_coreclkout} {clock} {slave};set_interface_property {pcie_256_hip_avmm_0_coreclkout} {EXPORT_OF} {pcie_256_hip_avmm_0_coreclkout_clock_bridge.in_clk};add_interface {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset} {reset} {slave};set_interface_property {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset} {EXPORT_OF} {pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge.in_reset};add_interface {pcie_256_hip_avmm_0_rd_dcm_master} {avalon} {slave};set_interface_property {pcie_256_hip_avmm_0_rd_dcm_master} {EXPORT_OF} {pcie_256_hip_avmm_0_rd_dcm_master_translator.avalon_anti_master_0};add_interface {pcie_256_hip_avmm_0_wr_dcm_master} {avalon} {slave};set_interface_property {pcie_256_hip_avmm_0_wr_dcm_master} {EXPORT_OF} {pcie_256_hip_avmm_0_wr_dcm_master_translator.avalon_anti_master_0};add_interface {pcie_256_hip_avmm_0_Txs} {avalon} {master};set_interface_property {pcie_256_hip_avmm_0_Txs} {EXPORT_OF} {pcie_256_hip_avmm_0_Txs_translator.avalon_anti_slave_0};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.Txs} {0};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.rd_dcm_master} {0};set_module_assignment {interconnect_id.pcie_256_hip_avmm_0.wr_dcm_master} {1};]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_DEVICE_FAMILY">
   <type>java.lang.String</type>
   <value>ARRIAV</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="AUTO_DEVICE">
   <type>java.lang.String</type>
   <value>5AGXFB3H4F35C5</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE</sysinfo_type>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>Arria V</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface
     name="pcie_256_hip_avmm_0_coreclkout"
     kind="clock_sink"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_coreclkout_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset"
     kind="reset_sink"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset_reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_rd_dcm_master"
     kind="avalon_slave"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>merlin.flow.avalon_universal_master_0</name>
    <value>avalon_universal_master_0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>18446744073709551616</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_address</name>
    <direction>Input</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_byteenable</name>
    <direction>Input</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_readdatavalid</name>
    <direction>Output</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_rd_dcm_master_writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
  </interface>
  <interface
     name="pcie_256_hip_avmm_0_wr_dcm_master"
     kind="avalon_slave"
     version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>merlin.flow.avalon_universal_master_0</name>
    <value>avalon_universal_master_0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>18446744073709551616</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>64</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_address</name>
    <direction>Input</direction>
    <width>64</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_byteenable</name>
    <direction>Input</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_readdatavalid</name>
    <direction>Output</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_wr_dcm_master_writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
  </interface>
  <interface name="pcie_256_hip_avmm_0_Txs" kind="avalon_master" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_coreclkout</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_address</name>
    <direction>Output</direction>
    <width>32</width>
    <role>address</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_read</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_readdata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_writedata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_byteenable</name>
    <direction>Output</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_readdatavalid</name>
    <direction>Input</direction>
    <width>1</width>
    <role>readdatavalid</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_waitrequest</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>pcie_256_hip_avmm_0_Txs_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>pcie_256_hip_avmm_0</moduleName>
    <slaveName>Txs</slaveName>
    <name>pcie_256_hip_avmm_0.Txs</name>
    <baseAddress>0</baseAddress>
    <span>4294967296</span>
   </memoryBlock>
  </interface>
 </module>
 <module
   name="rst_controller"
   kind="altera_reset_controller"
   version="14.0"
   path="rst_controller">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="NUM_RESET_INPUTS">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="OUTPUT_RESET_SYNC_EDGES">
   <type>java.lang.String</type>
   <value>deassert</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="SYNC_DEPTH">
   <type>int</type>
   <value>2</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQUEST_PRESENT">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQ_WAIT_TIME">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="MIN_RST_ASSERTION_TIME">
   <type>int</type>
   <value>3</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQ_EARLY_DSRT_TIME">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN0">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN1">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN2">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN3">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN4">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN5">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN6">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN7">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN8">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN9">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN10">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN11">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN12">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN13">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN14">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN15">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_INPUT">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ADAPT_RESET_REQUEST">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_CLK_CLOCK_RATE">
   <type>java.lang.Long</type>
   <value>-1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="reset_in0" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_in0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="clk" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>-1</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset_out" kind="reset_source" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>reset_in0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>reset_out</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
 </module>
 <module
   name="rst_controller_001"
   kind="altera_reset_controller"
   version="14.0"
   path="rst_controller_001">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="NUM_RESET_INPUTS">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="OUTPUT_RESET_SYNC_EDGES">
   <type>java.lang.String</type>
   <value>deassert</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="SYNC_DEPTH">
   <type>int</type>
   <value>2</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQUEST_PRESENT">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQ_WAIT_TIME">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="MIN_RST_ASSERTION_TIME">
   <type>int</type>
   <value>3</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQ_EARLY_DSRT_TIME">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN0">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN1">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN2">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN3">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN4">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN5">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN6">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN7">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN8">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN9">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN10">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN11">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN12">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN13">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN14">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN15">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_INPUT">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ADAPT_RESET_REQUEST">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_CLK_CLOCK_RATE">
   <type>java.lang.Long</type>
   <value>-1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="reset_in0" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_in0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="clk" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>-1</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset_out" kind="reset_source" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>reset_in0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>reset_out</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset</role>
   </port>
   <port>
    <name>reset_req</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
 </module>
 <module
   name="rst_translator"
   kind="altera_reset_translator"
   version="14.0"
   path="rst_translator">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="ACTIVE_LOW_RESET">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="SYNCHRONOUS_EDGES">
   <type>java.lang.String</type>
   <value>deassert</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQUEST_INPUT_ENABLE">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_CLK_CLOCK_RATE">
   <type>java.lang.Long</type>
   <value>-1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk" kind="clock_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>false</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>-1</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="in_reset" kind="reset_sink" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>in_reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
   <port>
    <name>reset_req_in</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
  <interface name="out_reset" kind="reset_source" version="14.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value>in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>out_reset</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
 </module>
 <connection
   name="clk_0.clk/alt_xcvr_reconfig_0.mgmt_clk_clk"
   kind="clock"
   version="14.0"
   start="clk_0.clk"
   end="alt_xcvr_reconfig_0.mgmt_clk_clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>alt_xcvr_reconfig_0</endModule>
  <endConnectionPoint>mgmt_clk_clk</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/pcie_reconfig_driver_0.reconfig_xcvr_clk"
   kind="clock"
   version="14.0"
   start="clk_0.clk"
   end="pcie_reconfig_driver_0.reconfig_xcvr_clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>pcie_reconfig_driver_0</endModule>
  <endConnectionPoint>reconfig_xcvr_clk</endConnectionPoint>
 </connection>
 <connection
   name="pcie_reconfig_driver_0.reconfig_mgmt/alt_xcvr_reconfig_0.reconfig_mgmt"
   kind="avalon"
   version="14.0"
   start="pcie_reconfig_driver_0.reconfig_mgmt"
   end="alt_xcvr_reconfig_0.reconfig_mgmt">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_reconfig_driver_0</startModule>
  <startConnectionPoint>reconfig_mgmt</startConnectionPoint>
  <endModule>alt_xcvr_reconfig_0</endModule>
  <endConnectionPoint>reconfig_mgmt</endConnectionPoint>
 </connection>
 <connection
   name="pcie_reconfig_driver_0.reconfig_busy/alt_xcvr_reconfig_0.reconfig_busy"
   kind="conduit"
   version="14.0"
   start="pcie_reconfig_driver_0.reconfig_busy"
   end="alt_xcvr_reconfig_0.reconfig_busy">
  <parameter name="endPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="width">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_reconfig_driver_0</startModule>
  <startConnectionPoint>reconfig_busy</startConnectionPoint>
  <endModule>alt_xcvr_reconfig_0</endModule>
  <endConnectionPoint>reconfig_busy</endConnectionPoint>
 </connection>
 <connection
   name="alt_xcvr_reconfig_0.cal_busy_in/pcie_reconfig_driver_0.cal_busy_in"
   kind="conduit"
   version="14.0"
   start="alt_xcvr_reconfig_0.cal_busy_in"
   end="pcie_reconfig_driver_0.cal_busy_in">
  <parameter name="endPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="width">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>alt_xcvr_reconfig_0</startModule>
  <startConnectionPoint>cal_busy_in</startConnectionPoint>
  <endModule>pcie_reconfig_driver_0</endModule>
  <endConnectionPoint>cal_busy_in</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/onchip_memory2_0.clk1"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="onchip_memory2_0.clk1">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>clk1</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/onchip_memory2_0.clk2"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="onchip_memory2_0.clk2">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>clk2</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.reconfig_to_xcvr/alt_xcvr_reconfig_0.reconfig_to_xcvr"
   kind="conduit"
   version="14.0"
   start="pcie_256_hip_avmm_0.reconfig_to_xcvr"
   end="alt_xcvr_reconfig_0.reconfig_to_xcvr">
  <parameter name="endPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="width">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>reconfig_to_xcvr</startConnectionPoint>
  <endModule>alt_xcvr_reconfig_0</endModule>
  <endConnectionPoint>reconfig_to_xcvr</endConnectionPoint>
 </connection>
 <connection
   name="alt_xcvr_reconfig_0.reconfig_from_xcvr/pcie_256_hip_avmm_0.reconfig_from_xcvr"
   kind="conduit"
   version="14.0"
   start="alt_xcvr_reconfig_0.reconfig_from_xcvr"
   end="pcie_256_hip_avmm_0.reconfig_from_xcvr">
  <parameter name="endPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="width">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>alt_xcvr_reconfig_0</startModule>
  <startConnectionPoint>reconfig_from_xcvr</startConnectionPoint>
  <endModule>pcie_256_hip_avmm_0</endModule>
  <endConnectionPoint>reconfig_from_xcvr</endConnectionPoint>
 </connection>
 <connection
   name="pcie_reconfig_driver_0.hip_currentspeed/pcie_256_hip_avmm_0.hip_currentspeed"
   kind="conduit"
   version="14.0"
   start="pcie_reconfig_driver_0.hip_currentspeed"
   end="pcie_256_hip_avmm_0.hip_currentspeed">
  <parameter name="endPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="width">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_reconfig_driver_0</startModule>
  <startConnectionPoint>hip_currentspeed</startConnectionPoint>
  <endModule>pcie_256_hip_avmm_0</endModule>
  <endConnectionPoint>hip_currentspeed</endConnectionPoint>
 </connection>
 <connection
   name="pcie_reconfig_driver_0.hip_status_drv/pcie_256_hip_avmm_0.hip_status"
   kind="conduit"
   version="14.0"
   start="pcie_reconfig_driver_0.hip_status_drv"
   end="pcie_256_hip_avmm_0.hip_status">
  <parameter name="endPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="endPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPort">
   <type>com.altera.entityinterfaces.IPort</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="startPortLSB">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="width">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_reconfig_driver_0</startModule>
  <startConnectionPoint>hip_status_drv</startConnectionPoint>
  <endModule>pcie_256_hip_avmm_0</endModule>
  <endConnectionPoint>hip_status</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/pcie_reconfig_driver_0.pld_clk"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="pcie_reconfig_driver_0.pld_clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>pcie_reconfig_driver_0</endModule>
  <endConnectionPoint>pld_clk</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.Rxm_BAR2/mm_interconnect_1.pcie_256_hip_avmm_0_Rxm_BAR2"
   kind="avalon"
   version="14.0"
   start="pcie_256_hip_avmm_0.Rxm_BAR2"
   end="mm_interconnect_1.pcie_256_hip_avmm_0_Rxm_BAR2">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>Rxm_BAR2</startConnectionPoint>
  <endModule>mm_interconnect_1</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_Rxm_BAR2</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/mm_interconnect_1.pcie_256_hip_avmm_0_coreclkout"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="mm_interconnect_1.pcie_256_hip_avmm_0_coreclkout">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>mm_interconnect_1</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_coreclkout</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.dma_rd_master/mm_interconnect_1.pcie_256_hip_avmm_0_dma_rd_master"
   kind="avalon"
   version="14.0"
   start="pcie_256_hip_avmm_0.dma_rd_master"
   end="mm_interconnect_1.pcie_256_hip_avmm_0_dma_rd_master">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>dma_rd_master</startConnectionPoint>
  <endModule>mm_interconnect_1</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_dma_rd_master</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_1.onchip_memory2_0_s1/onchip_memory2_0.s1"
   kind="avalon"
   version="14.0"
   start="mm_interconnect_1.onchip_memory2_0_s1"
   end="onchip_memory2_0.s1">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_1</startModule>
  <startConnectionPoint>onchip_memory2_0_s1</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>s1</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_1.pcie_256_hip_avmm_0_wr_dts_slave/pcie_256_hip_avmm_0.wr_dts_slave"
   kind="avalon"
   version="14.0"
   start="mm_interconnect_1.pcie_256_hip_avmm_0_wr_dts_slave"
   end="pcie_256_hip_avmm_0.wr_dts_slave">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_1</startModule>
  <startConnectionPoint>pcie_256_hip_avmm_0_wr_dts_slave</startConnectionPoint>
  <endModule>pcie_256_hip_avmm_0</endModule>
  <endConnectionPoint>wr_dts_slave</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_1.pcie_256_hip_avmm_0_rd_dts_slave/pcie_256_hip_avmm_0.rd_dts_slave"
   kind="avalon"
   version="14.0"
   start="mm_interconnect_1.pcie_256_hip_avmm_0_rd_dts_slave"
   end="pcie_256_hip_avmm_0.rd_dts_slave">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_1</startModule>
  <startConnectionPoint>pcie_256_hip_avmm_0_rd_dts_slave</startConnectionPoint>
  <endModule>pcie_256_hip_avmm_0</endModule>
  <endConnectionPoint>rd_dts_slave</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.dma_wr_master/mm_interconnect_2.pcie_256_hip_avmm_0_dma_wr_master"
   kind="avalon"
   version="14.0"
   start="pcie_256_hip_avmm_0.dma_wr_master"
   end="mm_interconnect_2.pcie_256_hip_avmm_0_dma_wr_master">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>dma_wr_master</startConnectionPoint>
  <endModule>mm_interconnect_2</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_dma_wr_master</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/mm_interconnect_2.pcie_256_hip_avmm_0_coreclkout"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="mm_interconnect_2.pcie_256_hip_avmm_0_coreclkout">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>mm_interconnect_2</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_coreclkout</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_2.onchip_memory2_0_s2/onchip_memory2_0.s2"
   kind="avalon"
   version="14.0"
   start="mm_interconnect_2.onchip_memory2_0_s2"
   end="onchip_memory2_0.s2">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_2</startModule>
  <startConnectionPoint>onchip_memory2_0_s2</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>s2</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.wr_dcm_master/mm_interconnect_3.pcie_256_hip_avmm_0_wr_dcm_master"
   kind="avalon"
   version="14.0"
   start="pcie_256_hip_avmm_0.wr_dcm_master"
   end="mm_interconnect_3.pcie_256_hip_avmm_0_wr_dcm_master">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>wr_dcm_master</startConnectionPoint>
  <endModule>mm_interconnect_3</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_wr_dcm_master</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/mm_interconnect_3.pcie_256_hip_avmm_0_coreclkout"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="mm_interconnect_3.pcie_256_hip_avmm_0_coreclkout">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>mm_interconnect_3</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_coreclkout</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.rd_dcm_master/mm_interconnect_3.pcie_256_hip_avmm_0_rd_dcm_master"
   kind="avalon"
   version="14.0"
   start="pcie_256_hip_avmm_0.rd_dcm_master"
   end="mm_interconnect_3.pcie_256_hip_avmm_0_rd_dcm_master">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>rd_dcm_master</startConnectionPoint>
  <endModule>mm_interconnect_3</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_rd_dcm_master</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_3.pcie_256_hip_avmm_0_Txs/pcie_256_hip_avmm_0.Txs"
   kind="avalon"
   version="14.0"
   start="mm_interconnect_3.pcie_256_hip_avmm_0_Txs"
   end="pcie_256_hip_avmm_0.Txs">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_3</startModule>
  <startConnectionPoint>pcie_256_hip_avmm_0_Txs</startConnectionPoint>
  <endModule>pcie_256_hip_avmm_0</endModule>
  <endConnectionPoint>Txs</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/pcie_reconfig_driver_0.reconfig_xcvr_rst"
   kind="reset"
   version="14.0"
   start="rst_controller.reset_out"
   end="pcie_reconfig_driver_0.reconfig_xcvr_rst">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>pcie_reconfig_driver_0</endModule>
  <endConnectionPoint>reconfig_xcvr_rst</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/alt_xcvr_reconfig_0.mgmt_rst_reset"
   kind="reset"
   version="14.0"
   start="rst_controller.reset_out"
   end="alt_xcvr_reconfig_0.mgmt_rst_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>alt_xcvr_reconfig_0</endModule>
  <endConnectionPoint>mgmt_rst_reset</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk_reset/rst_controller.reset_in0"
   kind="reset"
   version="14.0"
   start="clk_0.clk_reset"
   end="rst_controller.reset_in0">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk_reset</startConnectionPoint>
  <endModule>rst_controller</endModule>
  <endConnectionPoint>reset_in0</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/rst_controller.clk"
   kind="clock"
   version="14.0"
   start="clk_0.clk"
   end="rst_controller.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>rst_controller</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller_001.reset_out/onchip_memory2_0.reset1"
   kind="reset"
   version="14.0"
   start="rst_controller_001.reset_out"
   end="onchip_memory2_0.reset1">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller_001</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>reset1</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller_001.reset_out/onchip_memory2_0.reset2"
   kind="reset"
   version="14.0"
   start="rst_controller_001.reset_out"
   end="onchip_memory2_0.reset2">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller_001</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>reset2</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller_001.reset_out/rst_translator.in_reset"
   kind="reset"
   version="14.0"
   start="rst_controller_001.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller_001</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/mm_interconnect_1.onchip_memory2_0_reset1_reset_bridge_in_reset"
   kind="reset"
   version="14.0"
   start="rst_translator.out_reset"
   end="mm_interconnect_1.onchip_memory2_0_reset1_reset_bridge_in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>mm_interconnect_1</endModule>
  <endConnectionPoint>onchip_memory2_0_reset1_reset_bridge_in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller_001.reset_out/rst_translator.in_reset"
   kind="reset"
   version="14.0"
   start="rst_controller_001.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller_001</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/mm_interconnect_2.onchip_memory2_0_reset2_reset_bridge_in_reset"
   kind="reset"
   version="14.0"
   start="rst_translator.out_reset"
   end="mm_interconnect_2.onchip_memory2_0_reset2_reset_bridge_in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>mm_interconnect_2</endModule>
  <endConnectionPoint>onchip_memory2_0_reset2_reset_bridge_in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller_001.reset_out/rst_translator.in_reset"
   kind="reset"
   version="14.0"
   start="rst_controller_001.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller_001</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/mm_interconnect_3.pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset"
   kind="reset"
   version="14.0"
   start="rst_translator.out_reset"
   end="mm_interconnect_3.pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>mm_interconnect_3</endModule>
  <endConnectionPoint>pcie_256_hip_avmm_0_wr_dcm_master_translator_reset_reset_bridge_in_reset</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.nreset_status/rst_controller_001.reset_in0"
   kind="reset"
   version="14.0"
   start="pcie_256_hip_avmm_0.nreset_status"
   end="rst_controller_001.reset_in0">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>nreset_status</startConnectionPoint>
  <endModule>rst_controller_001</endModule>
  <endConnectionPoint>reset_in0</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/rst_controller_001.clk"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="rst_controller_001.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>rst_controller_001</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <connection
   name="pcie_256_hip_avmm_0.coreclkout/rst_translator.clk"
   kind="clock"
   version="14.0"
   start="pcie_256_hip_avmm_0.coreclkout"
   end="rst_translator.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>pcie_256_hip_avmm_0</startModule>
  <startConnectionPoint>coreclkout</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_pcie_reconfig_driver</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Altera PCIe Reconfig Driver</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>12</instanceCount>
  <name>clock_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Clock Input</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>10</instanceCount>
  <name>reset_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Input</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>11</instanceCount>
  <name>avalon_master</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Avalon Memory Mapped Master</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>20</instanceCount>
  <name>conduit_end</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Conduit</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>alt_xcvr_reconfig</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Transceiver Reconfiguration Controller</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>11</instanceCount>
  <name>avalon_slave</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Avalon Memory Mapped Slave</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>clock_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Clock Source</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>clock_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Clock Input</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>reset_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Input</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>clock_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Clock Output</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>reset_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Output</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_pcie_256_hip_avmm</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>V-Series Avalon-MM DMA for PCI Express</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>clock_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Clock Output</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>4</instanceCount>
  <name>reset_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Output</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_avalon_onchip_memory2</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>On-Chip Memory (RAM or ROM)</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>3</instanceCount>
  <name>altera_mm_interconnect</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>MM Interconnect</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>2</instanceCount>
  <name>altera_reset_controller</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Merlin Reset Controller</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_reset_translator</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Reset Translator</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>5</instanceCount>
  <name>clock</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Clock Connection</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>avalon</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Avalon Memory Mapped Connection</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>6</instanceCount>
  <name>conduit</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Conduit Connection</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>10</instanceCount>
  <name>avalon</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Avalon Memory Mapped Connection</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>6</instanceCount>
  <name>clock</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Clock Connection</displayName>
  <version>14.0</version>
 </plugin>
 <plugin>
  <instanceCount>12</instanceCount>
  <name>reset</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Reset Connection</displayName>
  <version>14.0</version>
 </plugin>
 <reportVersion>14.0 200</reportVersion>
 <uniqueIdentifier>1803730BB0E100000147A8BFD7EF</uniqueIdentifier>
</EnsembleReport>
