Intel Corporation
3065 Bowers Ave.
Santa Clara, CA 95051

contents of this ZIP file:

CAD File folder - Cadence Allegro(R) .brd file for this board
Schematic folder - Board schematic
Artwork folder - Fabrication drawings and artwork:

10/26/11
Artwork detail for Intel Corp. Boards:  G45491-003 and G45493-003

Board Number:  G45491-003 and G45493-003			Date:  OCT 26 2011
Plot Files:  13 of 13

Set Up Notes	

Gerber Type:  GERBER_RS274X		Film size:  36” x 24”
Scale:  1:1				Output units:  Inches
Format:  2.5				Coordinate type:  Absolute
Suppress Lead Zeroes:  Yes
Drill Code:  ASCII

File List

README.TXT		This Document

TOP.ART			Gerber data top signal layer
LAYER2.ART 		Gerber data internal plane layer
LAYER3.ART		Gerber data internal signal layer
BOTTOM.ART 		Gerber data bottom signal layer
SMT.ART			Gerber data solder-mask top
SMB.ART			Gerber data solder-mask bottom
SST.ART			Gerber data silkscreen top
SSB.ART			Gerber data silkscreen bottom
PMT.ART			Gerber data solder-paste top
PMB.ART			Gerber data solder-paste bottom
FAB1.ART		Gerber data fabrication drawing – sheet 1
FAB2.ART		Gerber data fabrication drawing – sheet 2
PANEL.ART		Gerber data pallete step and repeat – sheet 1

NCDRILL-1-4.DRL		NC Tape (drill) file
IPC356.IPC		IPC net list.

PCIE_GEN3_FAB_DWG1.PDF	PDF of fabrication drawing sheet 1
PCIE_GEN3_FAB_DWG2.PDF	PDF of fabrication drawing sheet 2
PCIE_GEN3_PANEL_DWG.PDF	PDF of panel drawing sheet 1