# _addcarry_u32(), _addcarry_u64()

Computes sum of two 32/64 bit wide unsigned integer values and a carry-in and returns the value of carry-out produced by the sum. The corresponding 4th Generation Intel® Core™ Processor extension instructions are `ADCX` and `ADOX`.

## Syntax

extern unsigned char _addcarry_u32(unsigned char c_in, unsigned int src1, unsigned int src2, unsigned int *sum_out);

extern unsigned char _addcarry_u64(unsigned char c_in, unsigned __int64 src1, unsigned __int64 src2, unsigned __int64 *sum_out);

## Parameters

c_in | Value used for determining carry-in value
src1 | 32/64 bit source integer
src2 | 32/64 bit source integer
*sum_out | Pointer to memory location where result is stored

## Description

The intrinsic computes sum of two 32/64 bit wide integer values, src1 and src2, and a carry-in value. The carry-in value is considered '1' for any non-zero c_in input value or '0' otherwise. The sum is stored to a memory location referenced by sum_out argument:

    *sum_out = src1 + src2 + (c_in !=0 ? 1 : 0)

### Note

This intrinsic does not perform validity checking of the memory address pointed to by sum_out, thus it cannot be used to find out if the sum produces carry-out without storing result of the sum.

## Returns

Returns the value of the intrinsic is a carry-out value generated by sum. The sum result is stored into memory location pointed by sum_out argument.

Parent topic: Intrinsics for Multi-Precision Arithmetic