# x, Qx

Tells the compiler which processor features it may target, including which instruction sets and optimizations it may generate.

## Syntax

Linux and macOS: | -x code

Windows: | /Qx code

## Arguments

code | Indicates to the compiler a feature set that it may target, including which instruction sets and optimizations it may generate. Many of the following descriptions refer to Intel® Streaming SIMD Extensions (Intel® SSE) and Supplemental Streaming SIMD Extensions (Intel® SSSE). Possible values are:
AMBERLAKE BROADWELL CANNONLAKE CASCADELAKE COFFEELAKE GOLDMONT GOLDMONT-PLUS HASWELL ICELAKE-CLIENT (or ICELAKE) ICELAKE-SERVER IVYBRIDGE KABYLAKE KNL KNM SANDYBRIDGE SILVERMONT SKYLAKE SKYLAKE-AVX512 TREMONT WHISKEYLAKE | May generate instructions for processors that support the specified Intel® processor or microarchitecture code name. Optimizes for the specified Intel® processor or microarchitecture code name. Keywords KNL and SILVERMONT are only available on Windows* and Linux* systems. Keyword ICELAKE is deprecated and may be removed in a future release.
COMMON-AVX512 | May generate Intel® Advanced Vector Extensions 512 (Intel® AVX-512) Foundation instructions, Intel® AVX-512 Conflict Detection instructions, as well as the instructions enabled with CORE-AVX2. Optimizes for Intel® processors that support Intel® AVX-512 instructions.
CORE-AVX512 | May generate Intel® Advanced Vector Extensions 512 (Intel® AVX-512) Foundation instructions, Intel® AVX-512 Conflict Detection instructions, Intel® AVX-512 Doubleword and Quadword instructions, Intel® AVX-512 Byte and Word instructions and Intel® AVX-512 Vector Length extensions, as well as the instructions enabled with CORE-AVX2. Optimizes for Intel® processors that support Intel® AVX-512 instructions.
CORE-AVX2 | May generate Intel® Advanced Vector Extensions 2 (Intel® AVX2), Intel® AVX, SSE4.2, SSE4.1, SSE3, SSE2, SSE, and SSSE3 instructions for Intel® processors. Optimizes for Intel® processors that support Intel® AVX2 instructions.
CORE-AVX-I | May generate Float-16 conversion instructions and the RDRND instruction, Intel® Advanced Vector Extensions (Intel® AVX), Intel® SSE4.2, SSE4.1, SSE3, SSE2, SSE, and SSSE3 instructions for Intel® processors. Optimizes for Intel® processors that support Float-16 conversion instructions and the RDRND instruction.
AVX | May generate Intel® Advanced Vector Extensions (Intel® AVX), Intel® SSE4.2, SSE4.1, SSE3, SSE2, SSE, and SSSE3 instructions for Intel® processors. Optimizes for Intel processors that support Intel® AVX instructions.
SSE4.2 | May generate Intel® SSE4 Efficient Accelerated String and Text Processing instructions, Intel® SSE4 Vectorizing Compiler and Media Accelerator, and Intel® SSE3, SSE2, SSE, and SSSE3 instructions for Intel® processors. Optimizes for Intel processors that support Intel® SSE4.2 instructions.
SSE4.1 | May generate Intel® SSE4 Vectorizing Compiler and Media Accelerator instructions for Intel® processors. May generate Intel® SSE4.1, SSE3, SSE2, SSE, and SSSE3 instructions for Intel processors that support Intel® SSE4.1 instructions.
ATOM_SSE4.2 | May generate MOVBE instructions for Intel® processors, depending on the setting of option -minstruction (Linux* and macOS*) or /Qinstruction (Windows*). May also generate Intel® SSE4.2, SSE3, SSE2, and SSE instructions for Intel processors. Optimizes for Intel Atom® processors that support Intel® SSE4.2 and MOVBE instructions. This keyword is only available on Windows* and Linux* systems.
ATOM_SSSE3 | May generate MOVBE instructions for Intel® processors, depending on the setting of option -minstruction (Linux* and macOS*) or /Qinstruction (Windows*). May also generate SSSE3, Intel® SSE3, SSE2, and SSE instructions for Intel processors. Optimizes for Intel Atom® processors that support Intel® SSE3 and MOVBE instructions. This keyword is only available on Windows* and Linux* systems.
SSSE3 | May generate SSSE3 and Intel® SSE3, SSE2, and SSE instructions for Intel® processors. Optimizes for Intel processors that support SSSE3 instructions. For macOS* systems, this value is only supported on Intel® 64 architecture. This replaces value T, which is deprecated.
SSE3 | May generate Intel® SSE3, SSE2, and SSE instructions for Intel® processors. Optimizes for Intel processors that support Intel® SSE3 instructions. This value is not available on macOS* systems.
SSE2 | May generate Intel® SSE2 and SSE instructions for Intel® processors. Optimizes for Intel processors that support Intel® SSE2 instructions. This value is not available on macOS* systems.
You can also specify Host. For more information, see option [Q]xHost.

## Default

Windows* systems: None Linux* systems: None macOS* systems: SSSE3 | On Windows systems, if neither /Qx nor /arch is specified, the default is /arch:SSE2. On Linux systems, if neither -x nor -m is specified, the default is -msse2.

## Description

This option tells the compiler which processor features it may target, including which instruction sets and optimizations it may generate. It also enables optimizations in addition to Intel feature-specific optimizations.

The specialized code generated by this option may only run on a subset of Intel® processors.

The resulting executables created from these option code values can only be run on Intel® processors that support the indicated instruction set.

The binaries produced by these code values will run on Intel® processors that support the specified features.

Do not use code values to create binaries that will execute on a processor that is not compatible with the targeted processor. The resulting program may fail with an illegal instruction exception or display other unexpected behavior.

Compiling the function main() with any of the code values produces binaries that display a fatal run-time error if they are executed on unsupported processors, including all non-Intel processors.

Compiler options m and arch produce binaries that should run on processors not made by Intel that implement the same capabilities as the corresponding Intel® processors.

The -x and /Qx options enable additional optimizations not enabled with options -m or /arch (nor with options -ax and /Qax).

On Windows systems, options /Qx and /arch are mutually exclusive. If both are specified, the compiler uses the last one specified and generates a warning. Similarly, on Linux and macOS* systems, options -x and -m are mutually exclusive. If both are specified, the compiler uses the last one specified and generates a warning.

### Note

All settings except SSE2 do a CPU check. However, if you specify option -O0 (Linux* or macOS*) or option /Od (Windows*), no CPU check is performed.

Product and Performance Information
Performance varies by use, configuration and other factors. Learn more at www.Intel.com/PerformanceIndex. Notice revision #20201201

## IDE Equivalent

Visual Studio: Code Generation > Intel Processor-Specific Optimization

Eclipse: Code Generation > Intel Processor-Specific Optimization

Xcode: Code Generation > Intel Processor-Specific Optimization

## Alternate Options

None

Parent topic: Code Generation Options

## See Also

xHost, QxHost compiler option
ax, Qax compiler option
arch compiler option
march compiler option
minstruction, Qinstruction compiler option
m compiler option