# _mm256_setr_epi32

Initializes 256-bit vector with integer values in reverse of specified order. No corresponding Intel® AVX instruction.

## Syntax

extern __m256i _mm256_setr_epi32(int, int, int, int, int, int, int, int); extern __m256i _mm256_setr_epi8(char e31, char e30, char e29, char e28, char e27, char e26, char e25, char e24, char e23, char e22, char e21, char e20, char e19, char e18, char e17, char e16, char e15, char e14, char e13, char e12, char e11, char e10, char e9, char e8, char e7, char e6, char e5, char e4, char e3, char e2, char e1, char e0); extern __m256i _mm256_setr_epi316(short e15, short e14, short e13, short e12, short e11, short e10, short e9, short e8, short e7, short e6, short e5, short e4, short e3, short e2, short e1, short e0); extern __m256i _mm256_setr_epi32(int e7, int e6, int e5, int e4, int e3, int e2, int e1, int e0); extern __m256i _mm256_setr_epi64x(__int64 e3, __int64 e2, __int64 e1, __int64 e0);

## Arguments

en | An 8/16/32/64-bit integer value to be initialized into the 256-bit vector. For each variant, there is one integer parameter for each 8/16/32/64-bit integer vector element.

## Description

Initializes a 256-bit vector with extended packed integer values (8/16/32/64-bit values), in reverse order, as specified by the en parameter.

## Returns

An 8/16/32/64-bit integer vector initialized with specified extended packed integer values in reverse.

Parent topic: Intrinsics for Miscellaneous Operations