# Intrinsics for Integer Move Operations

The prototypes for Intel® Advanced Vector Extensions 512 (Intel® AVX-512) intrinsics are located in the zmmintrin.h header file.
To use these intrinsics, include the immintrin.h file as follows:

    #include <immintrin.h>

Intrinsic Name | Operation | Corresponding Intel® AVX-512 Instruction
--- | --- | ---
`_mm512_mask_mov_epi32`, `_mm512_maskz_mov_epi32` | Move packed int32 elements. | `VMOVDQA32`
`_mm512_mask_mov_epi64`, `_mm512_maskz_mov_epi64` | Move packed int64 elements. | `VMOVQA64`

variable | definition
--- | ---
k | writemask used as a selector
a | first source vector element
src | source element to use based on writemask result

_mm512_mask_mov_epi32

    extern __m512i __cdecl _mm512_mask_mov_epi32(__m512i a, __mmask16 k, __m512i src);

Move packed int32 elements from a to destination using writemask k (elements are copied from src when the corresponding mask bit is not set).

_mm512_maskz_mov_epi32

    extern __m512i __cdecl _mm512_maskz_mov_epi32(__mmask16 k, __m512i a);

Move packed int32 elements from a to destination using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

_mm512_mask_mov_epi64

    extern __m512i __cdecl _mm512_mask_mov_epi64(__m512i a, __mmask16 k, __m512i src);

Move packed int64 elements from a to destination using writemask k (elements are copied from src when the corresponding mask bit is not set).

_mm512_maskz_mov_epi64

    extern __m512i __cdecl _mm512_maskz_mov_epi64(__mmask8 k, __m512i a);

Move packed int64 elements from a to destination using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Parent topic: Intrinsics for Move Operations