# Intrinsics for Blend and Conditional Merge Operations

Parent topic: Intrinsics for Intel® Advanced Vector Extensions

- _mm256_blend_pd
  Performs a conditional blend/merge of float64 vectors. The corresponding Intel® AVX instruction is VBLENDPD.
- _mm256_blend_ps
  Performs a conditional blend/merge of float32 vectors. The corresponding Intel® AVX instruction is VBLENDPS.
- _mm256_blendv_pd
  Performs conditional blend/merge of float64 vectors. The corresponding Intel® AVX instruction is VBLENDVPD.
- _mm256_blendv_ps
  Performs conditional blend/merge of float32 vectors. The corresponding Intel® AVX instruction is VBLENDVPS.