# Intrinsics to Determine Minimum and Maximum Values

Parent topic: Intrinsics for Intel® Advanced Vector Extensions

- _mm256_max_pd
  Determines the maximum of float64 vectors. The corresponding Intel® AVX instruction is VMAXPD.
- _mm256_max_ps
  Determines the maximum of float32 vectors. The corresponding Intel® AVX instruction is VMAXPS.
- _mm256_min_pd
  Determines the minimum of float64 vectors. The corresponding Intel® AVX instruction is VMINPD.
- _mm256_min_ps
  Determines the minimum of float32 vectors.The corresponding Intel® AVX instruction is VMINPS.