# _mm256_stream_load_si256

Loads 256-bit data from memory using non-temporal aligned hint. The corresponding Intel® AVX2 instruction is VMOVNTDQA.

## Syntax

extern __m256i _mm256_stream_load_si256(__m256i const *);

## Arguments

s1 | integer source vector used for the operation.

## Description

Loads 256-bit data from the source operand to the destination operand using a non-temporal hint if the memory source is write combining memory type.

Parent topic: Intrinsics for Miscellaneous Operations